IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.18:  5/09/2021 15:45:13

Lader Prof-181X  Format #8 

Track 0-1 beidseitig.  Daten sind nur auf Side 0

Required cylinders: 2
Required heads    : 2
Data rate         : 500kbps
Est. maximum track: 9040 bytes

Possible drives/options to write P181_LDR.IMD :

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

 5.25" HD 80-track
   Double-step: OFF

 8" 77-track
   Double-step: OFF

*1 Should fit on 360rpm drive, 300rpm drive will leave long end gap.
