# SDLTRS and the Videogenies

( German text )

There are various emulators for the TRS-80 (and other models) from Tandy. Unfortunately, little is known about the computers from EACA and TCS that are compatible with Tandy and are manufactured and distributed in Germany. These are only partially supported in the well-known emulators.I use Jens Guenter's emulator SDLTRS for the demonstration. Unfortunately, pictures of the screens of the original systems are much more difficult to take with a digital camera and are not always visually appealing. I also don't have all the systems presented here in my collection, which is why they can only be shown in the emulation. Please read the SDLTRS online documentation. All files are included in sdltrs_und_die_videogenies.7z so that the examples can also be tried out locally. I have tested the calls under Windows 10-64bit, if a 32bit Windows is used, SDL2TRS64.EXE must be replaced with SDL2TRS.EXE in the calls.

And yes, EACA made even the Colour Genie. But this one doesn't belong to the true TRS-80 compatibel systems, but a lot code in the ROM of the Colour Genie comes from the Video Genie. For the Colour Genie there are spezial emulators found on the web. I prefer the "CGENIE - The EG 2000 Colour Genie Emulator" from Jürgen Buchmüller (Pullmoll) running with MSDOS and real floppydrives.

Contents:

Genie I/II G-DOS NEWDOS H(acktory)-DOS Schmidtke CP/M

Genie III G-DOS2.1 G-DOS2.4 Kaempf CP/M Holte CP/M Lowe CP/M

Speedmaster

Genie IIs Kaempf CP/M G. Schroeder CP/M Grafik

Genie IIIs Holte CP/M Kaempf CP/M 2.x Kaempf CP/M 3 G-DOS 2.4 Grafik und RDLBASIC

The Video Genie

The best known is probably the video Genie I - also known as EG 3003. The Video Genie I had a cassette recorder installed, the Video Genie II had a 10-key keyboard instead of the cassette recorder. Information on all EACA / TCS computers can be found here, with the majority of the documentation being in German language. EACA has distributed the Video Genie as a TRS-80 compatible Computer Genie I/II in Europe. Other names were chosen in other countries.In Australia and New Zealand, for example, under the name System-80. The Genie computers were produced by the company EACA in Hong Kong and were distributed in Germany by the company TCS (Trommeschläger Computer Service). TCS offered extensive peripherals for the Genie I/II computers. The TCS Video Genie was also known as the "Video Genie System".
Video Genie I (https://www.video-genie.funkenzupfer.de/)
Video Genie II (https://www.video-genie.funkenzupfer.de/)

The Video Genie was originally delivered with NEWDOS-80.But then there was G-DOS (a germanized and expanded NEWDOS) and with various extensions to the 64-character mode, the 80-character mode and "high-resolution" graphics. With a banking adapter and memory expansion (necessary for the older models), CP/M was also available and possible as operating system.
Emulation for G-DOS with german character set:
`[g1_gdos22_charset1-genie.cmd]:`
`sdl2trs64 -rom vg1-TCS-rom.bin -charset1 genie -disk0 flogd02.dmk`
and for NEWDOS:
`[g1_newdos.cmd]:`
`sdl2trs64 -rom vg1-TCS-rom.bin -disk0 flond62.dmk`
There were also various adjustments to NEWDOS / G-DOS in the user groups of the time.

Here are the adaptations by Arnulf Sopp which he called H(acktory)-DOS. The H-DOS 2.3c supports the "EG-64 MBA (Memory-Banking Adapter" from TCS and this is also emulated with SDLTRS. The command B? displays the corresponding RAM banks of the EG-64 MBA. See also the german documentation for HDOS.

`[g1_hdos.cmd]:`
`sdl2trs64 -rom vg1-TCS-rom.bin -charset1 genie -disk0 hdos23c.dmk`
In addition to NEWDOS and GDOS, LSDOS or TRSDOS are also available as operating systems. The calls are according to the examples above. However, I mostly used NEWDOS or GDOS.
The following applies to the German character set:

In SDLTRS: Press ALT-I, select "Model I Character Set" and there select "Genie", with ENTER, TAB or SPACE confirm and press ESC... or on the command line with the option -charset1 genie ...
This character set is then used:
/* CG 10 - german charset for Genie I/II & Video Genie from: http://oldcomputers-ddns.org/public/pub/rechner/eaca/genie_1/roms/vg1_mit_tcs-expansion/tcs-rom-ext_zeichensatz_2716.bin */
With the option of memory expansion and/or bank switching, CP/M 2.2 was also possible, giving access to another large software area. Since port 0xFE got a bit "tight" for the emulator, there are a few changes:

The option for "CP/M-Banking" (Mattes/Schmidtke) is:
-speedup cpm, while the clock frequency remains at 1.78 MHz: it becomes a bit more "cozy"
- with -speedup lnw the LNW80 emulation is activated: 4 MHz and "fade in" the HRG into the lower 16K

Schmidtke CP/M - BIOS by Günter Ermer for the Videogenie
`[g1_schmidtke-cpm.cmd]:`
`sdl2trs64 -rom vg1-TCS-rom.bin -charset1 genie -speedup banking -disk0 flocpm01.dmk`

With the Schmidtke CP/M for the Videogenie the driver for the 80-Z card can be installed with `copy sys.sys=sys80.sys`. After a "cold start" with SHIFT-F10, this is then activated and 80*22 characters are displayed. In the Schmidtke-CP/M, the keyboard layout has been changed somewhat: the colon is on SHIFT-0 (function key F6 in SDLTRS), the semicolon is replaced in the "original" by SHIFT + SPACEBAR + ;, in SDLTRS this is currently only possible via the "Virtual Keyboard": ALT + J and select Keyboard there.

Below is 64 char mode, right is 80char mode.
Bios from Eberhard Mattes (thanks for the EMX on OS/2).
`[g1_schmidtke_cpm_mattes.cmd]:`
`sdl2trs64 -rom vg1-TCS-rom.bin -charset1 genie -speedup banking -disk0 flocpm02.dmk`
That's for the Video Genie I (Video Genie System).
Other computers were also developed by TCS and EACA. All of them run the operating systems known from the TRS-80, including CP/M on the Genie IIs, Genie III, Speedmaster and Genie IIIs models.

Genie III

(Pictures from: https://www.video-genie.funkenzupfer.de/)
The Genie III is TRS-80 compatibel running NEWDOS, G-DOS and CP/M.
`[g3_gdos_2.1.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk0 g3gd21-1.dmk`
`[g3_gdos_2.4.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk0 g3gd24-1.dmk`
CP/M for the III was made by Klaus Kaempf, Thomas Holte and Lowe Elecronics.
Klaus Kaempf is allready activ and his CP/M-Version 2.2X for the Genie IIs and the Genie III is on gitlab available.
CP/M 2.2 from Klaus Kaempf:
`[g3_kaempf_cpm.cmd]:`
`dl2trs64.exe -rom g3_sysrom_5100-01_2716_save.bin -disk0 cpm-2_2XV3-for-GenieIII.jv3`
Thomas Holte made a CP/M 2 and a CP/M 3 (Plus). CP/M 3 bis banked with emulating the G3PLUS card which expand memory to 384kb.
For the Holte CP/M there is the 'Holte-BIOS-ROM' needed. See how to add it to the real Genie III.
CP/M 2.2 from Thomas Holte:
`[g3_cpm2_holte.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk0 hv22d_01.dmk -serial ""`
CP/M 3 banked from Thomas Holte (emulatet with the GeniePLUS card and on the right as the card is really missing nonebanked) :
`[g3_cpm3-holte.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk0 g3-gplus.dmk -serial ""`
I like to use NZCOM with CP/M 2.x (a ZCPR enhancemend for CP/M) or Z3PLUS with CP/M 3.x
`[g3_holte_nzcom.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk1 hv22d-02.dmk -disk0 hv22d-03.dmk`
CP/M 2.2 from LOWE Electronics:
`[g3_cpm2_lowe.cmd]:`
`sdl2trs64.exe -rom g3_holte_eprom.bin -disk0 g3lowe01.dmk -serial ""`
Speedmaster and the Genie IIs
The Genie IIs and the Speedmaster use a backplane and cards in ECB format but are not compatibel to the ECB bus..
The Speedmaster has a 19" frame, der Genie IIs has a frame like teh Genie IIIs.
Speedmaster

``[speedmaster.cmd:]``
sdl2trs64.exe -rom speedm.rom tcs -doubler both -disk0 speedm.dmk -speedup tcs``

CP/M 2.2a from Thomas Holte

`
`

Genie IIs (picture from the TCS flyer)
Genie IIs CP/M Klaus Kaempf:
`[g2s_cpm22x_kaempf.cmd:]`
`sdl2trs64 -rom vg1-tcs-rom.bin -doubler percom -speedup tcs -disk0 g2s-cpm22x.dmk`
Genie IIs grafik in G-DOS 2.4 with RDLBASIC

Genie IIs with the CP/M from Gerald Schroeder. Gerald Schroeder replaced the Z80 with a moderne HD64180 and build the CP/M for his system.

`[g2s_gs_cpm.cmd:]`
`sdl2trs64.exe -rom speedm.rom -disk0 g2s-gs-cpm.dmk -doubler both -speedup tcs`

As of the special hardware and using a terminal over rs232 connection in this emulating is no cursor seen but the system is running.

Genie IIIs
The Genie IIIs is my favorite system. Speed is like the Genie IIs and Speedmaster. In the picture is the clamshell (IBM clone like) from ORGADATA.
Orgadata modificated the Genie IIIs to use 1.2MB PC floppydrives, but the possibility of connecting 4 x 8" drives was lost.
The Genie IIIs could use 4x5.25" and 4x8" floppydrives without modifications.

Below the Genie IIIs from TCS with the metallcase of 1mm dickness. The picture is from the TCS flyer as my Genie IIIs is open at the moment.

CP/M 3 from Thomas Holte:
`[g3s-cpm3_holte.cmd]:`
`sdl2trs64 -rom g3s_8501004_bootrom_2732.bin -disk0 g3s-h-f1.dmk -disk1 g3s-holte_jens.dmk`
CP/M 2.2 from Klaus Kaempf:
`[g3s-cpm2_kk.cmd]:`
`sdl2trs64 -rom g3s_8501004_bootrom_2732.bin -disk0 g3s_f09.dmk`
CP/M 3 from Klaus Kaempf:
`[g3s-cpm3_kk.cmd]:`
`sdl2trs64 -rom g3s_8501004_bootrom_2732.bin -disk0 escpm010.dmk`
In the above image Z3PLUS is starting automatically - no profile.sub is needed
G-DOS 2.4 Masterdisk for Genie IIS, Genie III and Genie IIIs
The systemdisks vor the seperate Genie type will be made with:
DO GDOSIIS [enter] oder DO GDOSIIIS [enter] oder DO GDOSIII [enter]
Only the device specific DOS will be copied to the floppydisk in drive 1.
`[g3s_gdos24_master.cmd]:`
`sdl2trs64 -rom g3s_8501004_bootrom_2732.bin -disk0 gdos24_master_char.dmk`
Directory shown in 80 char mode.
Genie IIIs G-DOS 2.4
Below G-DOS 2.4 made from the masterdisk for Genie IIIs with only files for the Genie IIIs on floppydisk.
`[g3s_gdos24.cmd]:`
`sdl2trs64 -rom g3s_8501004_bootrom_2732.bin -disk0 g3s-gdos24.dmk`
G-DOS 2.4 below in 64 char mode and right with 80 char.
Directory in 80 char mode with clock enabled:
RDLBASIC was enhanced for "high-resolution" graphics. Below some examples using RDLDEMO/JOB - start it with DO RDLDEMO
German Documentation for G-DOS 2.4