; AN FCB HAS THE FOLLOWING MEMORY MAP
;
;	DEFB		MODE	  (1 READ/ 2 WRITE/ 3 READWRITE 0 AVAILABLE
;	DEFW		POSITION IN FILE
;	DEFW
;	DEFS	32	FCB
;	DEFB		CURRENT RECORD
;	DEFW		RANDOM RECORD COUNT
;	DEFB		RANDOM RECORD OVERFLOW

FCBL	EQU	41
;RTN	EQU	0
;RTNL	EQU	RTN+2
;RTNA	EQU	RTNL+2
OLDS	EQU	0
RTNA	EQU	OLDS+2
ARG1	EQU	RTNA+2
ARG2	EQU	ARG1+2
ARG3	EQU	ARG2+2
