DIR Ver. 1.45-Aug 17 2020, Copyright 1996-2020, Sydex.  All rights reserved.
CR Decision Mate V - DSDD 48 tpi 5.25" - 512 x 8 format

MV Diagnostic Diskette 1.0


B0:ATIME1.COM      B0:BRUN.COM        B0:CONFIG.COM      B0:LATER.COM
B0:MENU1.COM       B0:PIP.COM         B0:RTCD6.COM       B0:V1K215.COM
B0:V1K216.COM      B0:V1K223.COM      B0:V1K233.COM      B0:V1K801.COM
B0:V1K803.COM      B0:V1K804.COM      B0:V1K806.COM

#########################################################

   DMV DIAGNOSTIC DISKETTE VERSION 01.00
                                                                                
   SELECT ONE OF THE FOLLOWING TESTS:                                           
                                                                                
   1. K215 - RS-232C BUFFERED SERIAL INTERFACE (MODEM)                          
   2. K216 - SERIAL COMMUNICATION CONTROLLER                                    
   3. K223 - DLC INHOUSE PRIMARY INTERFACE ADAPTER                              
   4. K233 - SHARED RAM                                                         
   5. RS 232 ADAPTERS K211, K212, K213, K801                                    
   6. K803 - REAL TIME CLOCK ADAPTER - DIAGNOSTIC PROGRAM                       
   7. K803 - REAL TIME CLOCK ADAPTER - DISPLAY PROGRAM                          
   8. K804 - IEEE-488 INTERFACE                                                 
   9. K806 - MOUSE INTERFACE                                                    
   A. K232 - NUMERIC COPROCESSOR                                                
   B. K234 - 68008 PROCESSOR CARTRIDGE                                          
                                                                                
   C. CONFIG                                                                    

