Usage of the FAX/Data Modem Test
================================

The FAX/Data Modem Test Program runs under the Operating Systems
PenOS or PenDOS. You will need a Flex Disk Drive or a connection to
a Computer with a Flex Disk Drive in order to copy the Modem Test
to your Notepad. You need to have a NCR FAX/Data Modem Card installed
which shall be tested. If you want to test the connection to another
computer the Modem must be connected to a Remote System.

In order to run the FAX/Data Modem Test the following steps must be
done:
   - copy the Test to the mass storage media in your NCR Notepad 3125
     (Fixed Disk / FLASH Disk / IC-Card).
   - install the Modem Card and evtl. connect to a Telephon Line.
   - run the Test.
   - evtl. delete the Test from the mass storage media in your
     Notepad.


Copy the Test Program to the Notepad
------------------------------------

The copy procedure depends on whether you copy the Test from a Flex
Disk Drive connected to the Notepad or copy it via serial or parallel
link (e.g. LAPLINK).


   = copy the Test from the Flex Disk Drive:

While in the NCR Notepad 3125 a Flex Disk Adapter  OR  a Modem can be
installed, the following procedure must be followed:

   - switch your computer off (Power Off).
   - properly install a Flex Disk Adapter and Flex Disk Drive. Refer
     to the Installation Instruction which came with the Flex Drive
     Kit.
   - start the computer again and call Setup (CTRL-ALT-S).
   - enable the Flex Disk Drive.
   - be sure to remove any Flex Disk from the Flex Disk Drive to Boot
     from the mass storage media (Fixed Disk / FLASH Disk / IC-Card).
   - insert the Diagnostic Diskette into the Flex Disk Drive.
   - if you have a GERMAN Modem:
        copy A:\MODEMTST\DEUTSCH\MODEMDEU.EXE to a working subdirectory
        on your mass storage media.
            Example:  COPY A:\MODEMTST\DEUTSCH\MODEMDEU.EXE C:\DIAG
   - if you have an US Modem:
        copy A:\MODEMTST\ENGLISH\MODEMENG.EXE to a working subdirectory
        on your mass storage media.
            Example:  COPY A:\MODEMTST\ENGLISH\MODEMENG.EXE C:\DIAG
   - invoke the Setup (CTRL-ALT-S).
   - disable the Flex Disk Drive.
   - switch your computer off.
   - remove the Flex Disk Adapter and properly install the FAX/Data
     Modem Card. Refer to the Installation Instruction which came with
     the FAX/Data Modem Kit.
   - start the computer again.


   = copy the Test via serial or parallel Link:

Refer to the Instruction Manual of the Transfer Software you are
using.

   - connect the Source Computer with the Notepad using the serial or
     parallel cable which came with the Transfer Software.
   - insert the Diagnostic Diskette into the Flex Disk Drive of the
     Source Computer.
   - start the Transfer Software on both computers (e.g. LAPLINK).
   - establish the connection.
   - set the Destination Path to a working subdirectory on the mass
     storage media of your Notepad.
        Example: C:\DIAG
   - if you have a GERMAN Modem:
        set the Source Path to the subdirectory \MODEMTST\DEUTSCH\
        of the Diagnostic Disk.
        Transfer the file MODEMDEU.EXE to the working subdirectory.
   - if you have an US Modem:
        set the Source Path to the subdirectory \MODEMTST\ENGLISH\
        of the Diagnostic Disk.
        Transfer the file MODEMENG.EXE to the working subdirectory.


NOTE: Be sure to use the appropriate FAX/Data Modem Test Program
      for your Country specific Version of the Modem Card.


Install the FAX/Data Modem Card
-------------------------------

Be sure to install the FAX/Data Modem Card properly to your NCR
Notepad 3125. If you additionally want to test the connection to
another computer connect the Modem properly to a Remote System.


Run the FAX/Data Modem Test
---------------------------

   - change the current subdirectory to the drive and working
     subdirectory on the Notepad which contains your FAX/Data
     Modem Test Program.
        Example: CD \DIAG
   - for normal Test Operation:
        + if you have a GERMAN Modem:
          invoke the Test by typing "MODEMDEU" followed by the Enter-
          Key at the DOS-Prompt.
        + if you have an US Modem:
          invoke the Test by typing "MODEMENG" followed by the Enter-
          Key at the DOS-Prompt.
   - if you additionally want to test the connection to a Remote
     System:
        + if you have a GERMAN Modem:
          invoke the Test by typing "MODEMDEU /ANW" followed by the
          Enter-Key at the DOS-Prompt.
        + if you have an US Modem:
          invoke the Test by typing "MODEMENG /DIAL" followed by the
          Enter-Key at the DOS-Prompt.
   - follow the instructions of the Test Program displayed on the
     screen.


Delete the FAX/Data Modem Test Program
--------------------------------------

When you do not longer need the FAX/Data Modem Test Program on the
mass storage media of your notepad you should delete the Test
Program file from the working subdirectory.

   - change the current subdirectory to the drive and working
     subdirectory on the Notepad which contains your FAX/Data
     Modem Test Program.
        Example: CD \DIAG
   - if you have a GERMAN Modem:
        type "DEL MODEMDEU.EXE" followed by the Enter-Key at the
        DOS-Prompt.
   - if you have an US Modem:
        type "DEL MODEMENG.EXE" followed by the Enter-Key at the
        DOS-Prompt.
