; PAR - FILE FOR MASTER SYSTEM
;
EOPCHR  = 0x7F      ;END OF PRINT CHARACTER
NMBUFS  = 0x18      ;NUMBER OF BUFFERS (24)
BUFSIZ  = 04        ;BUFFER SIZE 2 KB
OSMTOP  = (0x3000)  ;TOP OF MEMORY FOR DYNAMIC WORKING STORAGE
BUFBAS  = (0x0400)  ;BASE ADDRESS OF BUFFER AREA
BUFLEN  = (0x0C00)  ;LENGTH OF BUFFER AREA
WSEG    = (0x0000)  ;BUS WINDOW SEGMENT ADDRESS
WFDOFF  = (0x0600)  ;FLEXIBLE DISK BUFFER OFFSET
WFXOFF  = (0x0E02)  ;FIXED DISK BUFFER OFFSET
NETOFF  = (0x2E10)  ;NETWORK BUFFER OFFSET
MEMTBL  = 01,(0x1000),(0x3FFF-0x1000) ;MEMORY SPECIFICATION TABLE
CLSCHR  = 0x5E      ;COMMAND LINE SEPARATOR IS (^)
CLPCHR  = ">"       ;COMMAND LINE PROMPT CHARACTER
SRHDRV  = 0xFF      ;SEARCH FOR COMMANDS ON SYSTEM DRIVE
COMPAT  = 0xB0      ;COMPATIBILITY FLAGS: PERMISSIVE, MIXED MODE, GLOBAL WRITE
AUTUSR  = 0x80      ;AUTOMATIC LOGON TO USER 0 (PRIVILEGED)
DSKAST  =           ;DISK ASSIGNMENT TABLE
          0x00,DSKDRA
          0x00,DSKDRB
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
          0xFF,(0)  ;NONEXISTENT DRIVE
NMBSLV  = 0x03      ;HIGHEST SLAVE NUMBER
NMBRPS  = 0x02      ;NUMBER OF PREALLOCATED REPLY PACKETS
NMBMBS  = 0x04      ;NUMBER OF PREALLOCATED MESSAGE BUFFERS
NMBSVC  = 0x02      ;NUMBER OF NETWORK SERVER PROCESSES
MAXRPS  = 0x02      ;MAXIMAL NUMBER OF REPLY MESSAGES
MAXMBS  = 0x04      ;MAXIMAL NUMBER OF MESSAGE BUFFERS
SLVTBL  =           ;SLAVE TABLE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
SSLTBL  = "123456789"        ;SLAVE SUFFIX LETTER TABLE
DCNTBL  =           ;DC NODE TABLE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
PTRAST  = 01,LSTDRB,00,LSTDRA;PRINTER ASSIGNMENT TABLE PRINTER A AND B
DSPPAT  = 1,2       ;DE-SPOOL PRINTER ASSIGNMENT TABLE 
LSTBRA  = 0x6A      ;PRINTER BAUD RATE
LSTBRB  = 0x6E      ;PRINTER BAUD RATE
NVTABA  = NTABD     ;NATIONAL VERSION TABLE FOR P5360-02 PRINTER
QUEAST  =           ;QUEUE ASSIGNMENT TABLE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
OSMLEN  = (0x1000)  ;LENGTH OF DYNAMIC WORKING STORAGE (64 KB)
