; PAR - FILE FOR SIMPLE SLAVE SYSTEM
;
EOPCHR  = 7F        ;END OF PRINT CHARACTER
CLSCHR  = 5E        ;COMMAND LINE SEPARATOR IS (^)
CLPCHR  = "'"       ;COMMAND LINE PROMPT CHARACTER
SRHDRV  = 0FF       ;SEARCH FOR COMMANDS ON SYSTEM DRIVE
ATNCHR  = "^_"      ;ATTENTION CHARACTER
SLRCHR  = 1E        ;SLAVE RESET CHARACTER (^^)
COMPAT  = 0B0       ;COMPATIBILITY FLAGS: PERMISSIVE, MIXED MODE, GLOBAL WRITE
WARMFN  = 0,"WARMSTRT","Z80" ;WARMSTART AUTOLOAD FILENAME FOR 8 BIT SLAVE
CLBLEN  = 4D        ;COMMAND LINE BUFFER LENGTH (ONE LINE)
SBIBSZ  = (20)      ;SIZE OF INPUT BUFFER FOR CHANNEL B
MAXMBS  = 2         ;MAXIMUM NUMBER OF MESSAGE BUFFERS
MAXRPS  = 1         ;MAXIMUM NUMBER OF REPLY MESSAGES
MEMRES  = (00C0)    ;RESERVED MEMORY ABOVE TPA
CONAST  = 1,CONDRA  ;CONSOLE ASSIGNMENT TABLE (CHANNEL B)
CONBR   = 8F        ;CONSOLE BAUDRATE
CONIND  = 0C2       ;CONSOLE PROTOCOL CCTXX
;PATCH 1 - TO MAKE OPTIMIZED CONSOLE STATUS FUNCTIONS TO RETURN
;          STATUS IN L-REG (AS WELL AS A-REG).
CINTRY + 22 = PATCH,44
PATCH = 21,00,00,7D,0C9
;PATCH 12 - TO CORRECT PROBLEMS IN T-FUNCTION 41 EXPLICIT NETWORK ROUTING.
NETREQ + 4F9 = 0FE,0FE,28,20,0F,0F,0F,0F,0E6,0F,0C8
NETREQ + 523 = 0C3,NETREQ+516
BIOSBT + 0C7 = 1B,3D,20,40,1B,47,44,"    PMU  80    ",1B,47,40,0D,0A,0A,0A,"TurboDOS Rel. 1.41/6",0D,0A
LCLERR - 3F = 0,0,0
LCLERR - 3B = 0,0,0
LCLERR - 35 = 0,0,0
LCLERR - 31 = 0,0,0
LCLERR - 2B = 0,0,0
