; PAR - FILE FOR MASTER SYSTEM
;
EOPCHR  = 7F        ;END OF PRINT CHARACTER
NMBUFS  = 10        ;NUMBER OF BUFFERS (16)
MEMRES  = (0500)    ;RESERVED MEMORY ABOVE TPA
MEMBLL  = (2400)    ;MEMORY BASE LOWER LIMIT
CLSCHR  = 5E        ;COMMAND LINE SEPARATOR IS (^)
CLPCHR  = ">"       ;COMMAND LINE PROMPT CHARACTER
SRHDRV  = 0FF       ;SEARCH FOR COMMANDS ON SYSTEM DRIVE
AUTUSR  = 80        ;AUTOMATIC LOGON USER NUMBER 0 IN MASTER
COMPAT  = 0B0       ;COMPATIBILITY FLAGS: PERMISSIVE, MIXED MODE, GLOBAL WRITE
DSKAST  =           ;DISK ASSIGNMENT TABLE
           000,DSKDRA
           001,DSKDRA
           001,DSKDRB
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
           0FF,(0)  ;NONEXISTENT DRIVE
FXDINB  = 01,32,04,00,84,00,80,0B     ;INITIALIZATION STRING FIXED DISK ST412
FXDSTB  = 85,20,0A,10,02,20,00,88,02,00,00 ;DISK SPECIFICATION STRING 10M FIXED
NMBSLV  = 4         ;NUMBER OF SLAVES
NMBRPS  = 4         ;NUMBER OF PREALLOCATED REPLY MESSAGES
MAXRPS  = 4         ;MAXIMUM NUMBER OF REPLY MESSAGES
NMBMBS  = 08        ;NUMBER OF PREALLOCATED MESSAGE BUFFERS
MAXMBS  = 08        ;MAXIMUM NUMBER OF MESSAGE BUFFERS
NMBSVC  = 4         ;NUMBER OF NETWORK SERVER PROCESSES
SLVTBL  =           ;SLAVE TABLE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
          00        ;SIMPLE SLAVE OR DC SLAVE
SSLTBL  = "123456789"        ;SLAVE SUFFIX LETTER TABLE
DCNTBL  =           ;DC NODE TABLE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
          00        ;SIMPLE, BATCH OR DC SLAVE
PTRAST  = 01,LSTDRA          ;PRINTER ASSIGNMENT TABLE PRINTER A ON CHANNEL B
LSTBRA  = 6F        ;PRINTER BAUD RATE
QUEAST  =           ;QUEUE ASSIGNMENT TABLE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
          00,(0)    ;LOCAL QUEUE
;THE FOLLOWING PATCH PREVENTS THE MASTER PROCESSOR FROM HANGING
;WHEN THERE IS NO AVAILABLE MEMORY FOR DYNAMIC BUFFERS
ALLOC + 86 = (2000)
;PATCH 1 - TO MAKE OPTIMIZED CONSOLE STATUS FUNCTIONS TO RETURN
;          STATUS IN L-REG (AS WELL AS A-REG).
CINTRY + 22 = PATCH,44
PATCH = 21,00,00,7D,0C9
