CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 1


SCREEN  1          INITIALIZATION                P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
     Do you want to install a new system    (0 - install)                      
     or update an existing system           (1 - update )  : 1                 
                                                                               
     Enter System Type         (0 - P3500,   1 - P3800  )  : 0                 
                                                                               
     Enter Master PMU Type     (1 - PMU80-1,            )                      
                               (2 - PMU80-3, 3 - PMU186 )  : 1                 
                                                                               
                                                                               
     Enter type and drive letter of the customer system disk                   
                                                                               
     Type :  1 - 5.25" flexible        4 - 5.25" fixed 20MB                    
             2 - 5.25" fixed  5MB      5 - 5.25" fixed 40MB                    
             3 - 5.25" fixed 10MB      6 - 8"    fixed 60MB                    
                                                                               
     Disk Type     (1..6) : 1          Drive Letter (A..P) : A                 
     Internal Disk (Y/N)  : Y                                                  
                                                                               
     Do you want to copy the relocatable files to the customer disk (Y/N) : N  




SCREEN  2          REGISTRATION                  P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
     TurboDOS serial number       : 16/31129                                   
     TurboDOS 12NC number         : 8702 402 10160                             
     Enter customer name          :                                            
     Enter engineers name         :                                            
     Enter branch office          :                                            
     Enter date (dd-mm-yy)        : 28-06-85                                   
                                                                               
                                                                               
     Remarks :                                                                 
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
                                                                               
CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 2


SCREEN  3          DISK ASSIGNMENT               P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
     Drive letter of first  5.25" flexible disk (A..P) : A                     
     Drive letter of second 5.25" flexible disk                                
     (A..P - if existent, 0 - if not existent)         : B                     
                                                                               
     Fixed Disk Types:   0 - NONE                  3 - 5.25" Fixed 20MB        
                         1 - 5.25" Fixed  5MB      4 - 5.25" Fixed 40MB        
                         2 - 5.25" Fixed 10MB      5 - 8"    Fixed 60MB        
                                                                               
                                                                               
     Fixed Disk      !  Disk  ! No of log.! Drive Letters of logical Volumes   
                     !  Type  !  Volumes  !             (A..P)                 
                     ! (0..5) !   (1..9)  ! 1 ! 2 ! 3 ! 4 ! 5 ! 6 ! 7 ! 8 ! 9  
     ----------------+--------+-----------+---+---+---+---+---+---+---+---+--- 
     First  Internal !    0   !           !   !   !   !   !   !   !   !   !    
     Second Internal !    0   !           !   !   !   !   !   !   !   !   !    
     External        !    2   !     1     ! C !   !   !   !   !   !   !   !    
                                                                               
     Drive letter of 8" flexible extension box                                 
     (A..P - if existent, 0 - if not existent)         : 0                     




SCREEN  4     MASTER PRINTER & QUEUE ASSIGNMENT  P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
     Printer Type :                            Protocol Type :                 
                                                                               
     0 - None                                  R - Ready/Busy                  
     1 - P2932/P2933/P2934                     X - Xon/Xoff                    
     2 - P2908/P2909                                                           
     3 - P5360 - 02                                                            
                                                                               
                                                                               
     Channel     !      Type     !        Baudrate         !   Protocol        
                 !     (0..3)    !    (See Help Screen)    !    (R/X)          
     ------------+---------------+-------------------------+-------------      
        A        !       0       !                         !                   
        B        !       1       !          19200          !      R            
                                                                               
                                                                               
     Number of spool queues (1..16) : 03                                       
                                                                               
     Do you want a communication channel driver (Y/N) : N                      
                                                                               
CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 3


SCREEN  5          SLAVE PROCESSORS              P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
     Slave Type :                             PMU Type :                       
                                                                               
     0 - None                                 0 - PMU80    2 - PMU88S (256KB)  
     1 - Simple Slave     3 - DC Node         1 - PMU186   3 - PMU88S (128KB)  
     2 - Batch Slave      4 - DC Slave                                         
                                                                               
       Slave   !   Type   ! PMU Type !  Slave   !   Type   ! PMU Type          
               !  (0..4)  !  (0..3)  !          !  (0..4)  !  (0..3)           
     ----------+----------+----------+----------+----------+----------         
         1     !    1     !    0     !    5     !          !                   
         2     !    1     !    0     !    6     !          !                   
         3     !    1     !    1     !    7     !          !                   
         4     !    1     !    1     !    8     !          !                   
               !          !          !    9     !          !                   
                                                                               
                                                                               
     Do you want to configure different slaves (Y/N) :  Y                      
                                                                               
                                                                               




SCREEN  6          SIMPLE SLAVE (processor 1)    P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
  Console Type :          Printer Type :                 Protocol Type :       
  0 - None                0 - None                       R - Ready/Busy (H0/T0)
  1 - P2711               1 - P2932/P2933/P2934          C - CCTXX             
  2 - P2705               2 - P2908/P2909                X - Xon/Xoff          
  3 - P3100               3 - P5360 - 02                                       
                                                                               
                                                                               
     Channel !  Console !  Printer  !  Modem  !      Baudrate     ! Protocol   
             !  (0..3)  !  (0..3)   !  (Y/N)  ! (See Help Screen) ! (R/C/X)    
     --------+----------+-----------+---------+-------------------+---------   
        A    !    0     !     0     !         !                   !            
        B    !    1     !     1     !    N    !       19200       !    C       
                                                                               
                                                                               
     Do you want a communication channel driver (Y/N) :  N                     
                                                                               
     Do you need a maximum TPA (only for 8 bit) (Y/N) :  Y                     
                                                                               
                                                                               
CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 4


SCREEN  6          SIMPLE SLAVE (processor 2)    P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
  Console Type :          Printer Type :                 Protocol Type :       
  0 - None                0 - None                       R - Ready/Busy (H0/T0)
  1 - P2711               1 - P2932/P2933/P2934          C - CCTXX             
  2 - P2705               2 - P2908/P2909                X - Xon/Xoff          
  3 - P3100               3 - P5360 - 02                                       
                                                                               
                                                                               
     Channel !  Console !  Printer  !  Modem  !      Baudrate     ! Protocol   
             !  (0..3)  !  (0..3)   !  (Y/N)  ! (See Help Screen) ! (R/C/X)    
     --------+----------+-----------+---------+-------------------+---------   
        A    !    0     !     0     !         !                   !            
        B    !    1     !     1     !    N    !       19200       !    C       
                                                                               
                                                                               
     Do you want a communication channel driver (Y/N) :  N                     
                                                                               
     Do you need a maximum TPA (only for 8 bit) (Y/N) :  Y                     
                                                                               
                                                                               




SCREEN  6          SIMPLE SLAVE (processor 3)    P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
  Console Type :          Printer Type :                 Protocol Type :       
  0 - None                0 - None                       R - Ready/Busy (H0/T0)
  1 - P2711               1 - P2932/P2933/P2934          C - CCTXX             
  2 - P2705               2 - P2908/P2909                X - Xon/Xoff          
  3 - P3100               3 - P5360 - 02                                       
                                                                               
                                                                               
     Channel !  Console !  Printer  !  Modem  !      Baudrate     ! Protocol   
             !  (0..3)  !  (0..3)   !  (Y/N)  ! (See Help Screen) ! (R/C/X)    
     --------+----------+-----------+---------+-------------------+---------   
        A    !    0     !     0     !         !                   !            
        B    !    3     !     1     !    N    !       19200       !    C       
                                                                               
                                                                               
     Do you want a communication channel driver (Y/N) :  N                     
                                                                               
     Do you need a maximum TPA (only for 8 bit) (Y/N) :                        
                                                                               
                                                                               
CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 5


SCREEN  6          SIMPLE SLAVE (processor 4)    P3000 CONFIG   8701 311 70610 
-------------------------------------------------------------------------------
                                                                               
  Console Type :          Printer Type :                 Protocol Type :       
  0 - None                0 - None                       R - Ready/Busy (H0/T0)
  1 - P2711               1 - P2932/P2933/P2934          C - CCTXX             
  2 - P2705               2 - P2908/P2909                X - Xon/Xoff          
  3 - P3100               3 - P5360 - 02                                       
                                                                               
                                                                               
     Channel !  Console !  Printer  !  Modem  !      Baudrate     ! Protocol   
             !  (0..3)  !  (0..3)   !  (Y/N)  ! (See Help Screen) ! (R/C/X)    
     --------+----------+-----------+---------+-------------------+---------   
        A    !    0     !     0     !         !                   !            
        B    !    1     !     1     !    N    !       19200       !    C       
                                                                               
                                                                               
     Do you want a communication channel driver (Y/N) :  N                     
                                                                               
     Do you need a maximum TPA (only for 8 bit) (Y/N) :                        
                                                                               
                                                                               




CONFIG  Release 6     S U M M A R Y  R E P O R T                    Page 6




CONFIG created the GEN and PAR files with the following defaults :
The command line separator character is ^ (circumflex)
The command line prompt character is >
The command line buffer length is 157 characters
Commands are searched on current drive first, then on system drive
The MASTER command logs on to user 0 in the master processor automatically
The user number for LOGOFF is 31
The number of NETSVC server processes is equal to the number of slaves (max. 5)
The number of buffers is 16
The buffer size is 1024 bytes
The attention character for the master is CTRL A
The attention character for a slave is CTRL underscore
The slave reset character is CTRL circumflex (type twice to reset slave)
The number of pre-allocated message buffers is equal to 2 * (number of slaves)
The number of pre-allocated reply packets is equal to the number of slaves 
The compatibility flag is set to 0B0: permissive, global write and mixed mode
Minimum Transient Program Area in the master is 8K
Minimum Transient Program Area in a 8 bit slave is 4K
The user sign-on message is: PHILIPS P3000 Release 6
