p35-005  Install CP/M3 von Janich & Klaas / MKC 
         --------------------------------------

BEGIN MIC7  Michels and Kleberhoff CP/M 3 - DSDD 96 tpi 5.25" - 512 x 10
DENSITY MFM ,LOW
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER EAGLE COMPLEMENT
BSH 4 BLM 15 EXM 0 DSM 394 DRM 127 AL0 0C0H AL1 0 OFS 2
END



CDIR Ver. 1.45-Aug 17 2020, Copyright 1996-2020, Sydex.  All rights reserved.
Michels and Kleberhoff CP/M 3 - DSDD 96 tpi 5.25" format

B0:BNKBDOS3.SPR    B0:CCP.COM         B0:CPM31.SYS       B0:CPM33.SYS       
B0:CPM35.SYS       B0:CPM36.SYS       B0:CPMINST.COM     B0:DISKCOPY.COM    
B0:DISKFORM.DAT    B0:FORMAT.COM      B0:GENCPM.COM      B0:LIB.COM         
B0:LINK.COM        B0:MAC.COM         B0:PIP.COM         B0:RESBDOS3.SPR    
B0:RMAC.COM        B0:SID.COM         B0:SUBMIT.COM      B0:V1801.CPM       
B0:V1803.CPM       

466K free on drive B:
