## Large picture of the LSI ADM3A

At the left you can see the DIP switches used for choosing the terminal configuration (baud rate etc). The keyboard is very solid and fells like some old typewriter :). The little turnknob below the screen at the right is used for adjusting the CRT brightness.

One interesting thing to note is that the picture at the screen changes its size a bit when one touches the screen due to the capacitive influence of the human body (seems like the picture somewhat "pumps" as one repeatedly touches the CRT).

Unfortunately the former screen content has somewhat burned in, though it is not that clearly visible "in real life" as seen on the picture, it seems the photo flash causes the burned letters to be more clearly visible.