IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.18: 15/06/2019 14:59:33

Prof 180X  CP/M3 Format #4 skew 5 | P180-3-2



CP/M 3 und Z3PLUS

Required cylinders: 80
Required heads    : 2
Data rate         : 300kbps
Est. maximum track: 6055 bytes

Possible drives/options to write P180-502.IMD :

 5.25" DD 40-track
   Double-step: OFF
   300 kbps -> 250 kbps

 5.25" QD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps

 5.25" HD 80-track
   Double-step: OFF

 3.5" DD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps

 3.5" HD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps
