IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.18: 31/03/2019 23:37:25

Prof 180X  CP/M 2.2 Systemdisk 

Required cylinders: 80
Required heads    : 2
Data rate         : 300kbps
Est. maximum track: 6055 bytes

Possible drives/options to write P180CPM2.IMD :

 5.25" DD 40-track
   Double-step: OFF
   300 kbps -> 250 kbps

 5.25" QD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps

 5.25" HD 80-track
   Double-step: OFF

 3.5" DD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps

 3.5" HD 80-track
   Double-step: OFF
   300 kbps -> 250 kbps
