IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.18: 28/10/2020 21:03:25

Prof-181X  Format 14 3.5" HD 1,44MB

Bootlader auf Systemspurem vorhanden



Mit NSWP, VDE 

Required cylinders: 80
Required heads    : 2
Data rate         : 500kbps
Est. maximum track: 10066 bytes

Possible drives/options to write FORMAT14.IMD :

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

 5.25" HD 80-track
   Double-step: OFF

*1 Should fit on 360rpm drive, 300rpm drive will leave long end gap.
