			--THE README FILE--
		      ------------------------

README contains late-breaking news and tips about WordStar,
and information about printers.


THE DISKS THAT CAME IN YOUR PACKAGE
-----------------------------------

The file HOMONYMS.TXT is included on the Speller disk
contrary to what is listed in Appendix D.


INSTALLATION
------------

WINSTALL and WSCHANGE

  WordStar has two installation programs:

  o  WINSTALL contains the basic choices to install WordStar.
     It is recommended for all users.

     Be sure and install your valid disk drives since WordStar 
     running under CP/M cannot recover from attempts to access non-
     existent disk drives.

  o  WSCHANGE contains every installation and customization
     choice.  It is designed for advanced users and users who
     want to customize WordStar after they're familiar with it.
     Use the menu listing below for a directory of the menus
     in WSCHANGE.

Directory of WSCHANGE Menus

  The chart below shows the organization of menus in WSCHANGE.
  Print it out and refer to it as you customize WordStar.

  Main Installation Menu

  A Console
    A Monitor
      A Monitor selection
      B Monitor name
      C Screen sizing
    B Function keys
    C Monitor patches
      A Special characters
      B Cursor control
      C Screen control
    D Keyboard patches
      A Function keys
      B Save function keys
    E Interface patches
      A Console busy handshaking
      B Special I/O subroutines
  B Printer
    A Printer choices
      A Printer selection
      B Printer name
      C Default printer driver
    B Printer driver library
      A Select library file
      B Create smaller library
      C Add new printer driver
      D Change printer driver data
    C WS printer patches
      A Custom print controls, printer initialization

  NOTE:  Disregard the "CUSTOM & SIMPLE Controls  Save CUSTOM/SIMPLE
  Controls" option shown.  This is not available from this menu.

    D Printing defaults
    E Printer interface
      A Printer port selection
      B Printer busy handshaking
      C Printer subroutines
  C Computer
    A Disk drives
      A Valid disk drives
      B Maximum valid user number
      C Delay disk access if typing
    B Operating system
      A Single-user system
      B Multi-user MP/M
      C Multi-user Turbo DOS
      D ZCPR3
    C Memory usage
    D WordStar files
    E Directory display
    F Computer patches
  D WordStar
    A Page layout
      A Page sizing & margins
      B Headers & footers
      C Tabs
    B Editing settings
      A Edit screen & help level
      B Typing
      C Paragraph alignment
      D Blocks
      E Erase & unerase
      F Lines & characters
      G Find & replace
      H WordStar 3.3 compatibility
      I Printing defaults
    C Other features
      A Spelling checks
      B Nondocument mode
      C Indexing
      D Shorthand (key macros)
      E Merge printing
      F Miscellaneous
  E Patching
    A Auto patcher
    B Save settings
    C Reset all settings

MEMORY USAGE
------------

  WordStar requires a minimum TPA size of 50 kbytes to run  
  using the factory defaults.  The TPA is the amount of memory  
  available in your computer for use by programs that have a  
  file type of COM.  To see how big the TPA is in your computer,
  press the question mark key (?) at the Opening Menu.

  The amount of memory required by WordStar can be reduced by 
  approximately 3 kbytes if necessary.  Use the WSCHANGE program 
  to select the minimum memory configuration option.  The menu  
  will show you what capabilities are being reduced.

  WordStar uses a general-purpose buffer for a variety of  
  tasks.  WordStar allocates memory to this buffer for editing,  
  for merge printing, and at the Opening Menu (see BFSIZE in 
  PATCH.LST).  The buffer used for editing is usually the most 
  sensitive to a reduced TPA size.  (You may be able to use the 
  Opening Menu and print, but there may be insufficient memory 
  for editing.)

  The merge print buffer is used only to hold merge print  
  variable names and data.  Increase it if you run out of memory 
  while merge printing.

  The  Opening Menu buffer is used primarily to hold the file 
  directory, and for miscellaneous tasks.


LOW-MEMORY INDICATOR IN STATUS LINE 
-----------------------------------

  If the Low-Memory indicator appears in the status line, it  
  means that WordStar was unable to complete some function.   
  The most common symptoms are:  the line number in the  
  status line is wrong, or a paragraph alignment could not be 
  completed. You may correct the line counter by saving your 
  file, exiting WordStar, and re-loading your file.  To correct 
  the paragraph alignment, move your cursor to the point where 
  paragraph alignment stopped, and then press ^B again.

  The reason this comes up is that WordStar was not able to fit  
  a big enough chunk of text into memory at one time.

  When you first begin editing, WordStar uses the value from 
  EDSIZE in the user area to determine the minimum amount  
  of memory required for a page of text.  The default  
  is set for approximately a 55 line by 66 column page.  If 
  your page size is routinely larger than this, you may want  
  to increase EDSIZE.  Multiply the number of lines by the 
  number of columns, and divide by 128.

  If the Low-Memory indicator comes on while printing, it is due 
  to either the same reasons as for editing, or there is  
  insufficient memory to print the text proportionally spaced.  
  The amount of memory required depends on which printer 
  driver you  are using.  If you aren't using the .PS ON dot 
  command to turn proportional spacing on in your document, 
  low memory won't be a problem.  Also, WordStar uses more 
  memory for merge printing than it does for regular printing 
  (around 2.5 kbytes more).

  The Low-Memory indicator will also appear when a full disk error
  is encountered during editing.  Treat the disk-full error as you
  would normally.


RAM-RESIDENT PROGRAMS
---------------------

  RAM-resident programs, such as SmartKey, reduce the amount of 
  working memory (TPA) that WordStar can use. The new features in 
  WordStar, such as shorthand, may reduce the need for these 
  RAM-resident programs, thus freeing memory for WordStar.


ZCPR3 SUPPORT
-------------

  In order to enable the ZCPR facilities within WordStar, the user 
  must use the Z3INS utility provided with ZCPR to install the 
  address of the ZCPR "environment" into WordStar. The environment 
  contains information that WordStar uses to support ZCPR-specific 
  functions.
  
  Generally, the user should log onto the drive containing the file 
  WS.COM, and issue the command:
  
  	Z3INS SYS.ENV WS.COM
  	
  The user should also run either WINSTALL or WSCHANGE to further 
  install WordStar for ZCPR. However, this is not mandatory because 
  the only thing that happens is that the WordStar sign-on says 
  "ZCPR3," and the LGLUSR location in the user area is changed for a 
  maximum user number of 31. (The normal default for LGLUSR is 15.)
  
  Once the user has installed WordStar for use with ZCPR, the user 
  will be able to use the following ZCPR features:
  
  - A named directory may be used when logging onto a new drive/user.
  	
  - A named directory may be used instead of a drive/user as part
    of any file name.
  	  
  - The drive/user always appears above file directories. (For CP/M
    only the drive letter is shown if the user number is zero.)
  	  
  - The directory name also appears above the directory if one has
    been defined for the currently logged drive/user.
  	  
  - If WordStar does not find its OVR files on the current drive and
    user, it will search the drives and user numbers in the ZCPR
    search path rather than using its standard search pattern.
  	  
  - WordStar installs itself as a ZCPR "shell" process which lets the
    user enter any legal ZCPR command when running a program. (CP/M
    can only run programs that are COM files.)


OSBORNE USERS
-------------

  The command to change a hard carriage return to a soft carriage
  return (document mode) or to turn Auto-indent ON (nondocument
  mode) does not function on the Osborne because of a limitation
  in its BIOS.  The following patch can be applied to change the
  command from ^^ to ^- (Ctrl-Hyphen):

  Using DDT or SID in the file WSMSGS.OVR:

	At 02DA replace 1E with a 1D
	At 02EF replace 1E with a 1D
	At 0359 replace 1E with a 1D
	At 06B2 replace 1E with a 1D
	At 06C9 replace 1E with a 1D

  At the system prompt type SAVE 53 WSMSGS.OVR

  For more information on how to use SID or DDT, see your CP/M
  reference guide.  As always, be sure and apply the patch to a
  COPY of the file.


INSTRUCTIONS FOR TWO FLOPPY DISK COMPUTERS
------------------------------------------

  Do not remove the Program disk while you are using WordStar.

  The Printer Driver Library file (WSPRINT.OVR) on the WordStar 
  program disk is much smaller than the Printer Driver Library 
  file contained on the disk labeled PRINTER. Be sure to read the 
  section in "Starting" that discusses the printer library file.


RUN A PROGRAM
-------------

  Once you press R you can type the drive and user number for the 
  program you want to run. You may run only .COM files. CCP commands, 
  such as DIR cannot be used. 


INDEXING
--------

Using StarIndex

  StarIndex 1.01 works with files created with this release of
  WordStar.  

"Can't Use That Printer" Message

  When WordStar creates an index or table of contents, it uses
  the printer drivers $INDEX and $TOC.  If you created a smaller
  WSPRINT.OVR file, you may have left these drivers out.  To
  return them to the file, copy the original WSPRINT.OVR file
  onto your disk.  When you create a smaller file again, be sure
  to save these drivers.  See Appendix C in the WordStar manual 
  for a list of other drivers to save.


SPELL CHECKING
--------------

  Dual floppy disk users:
  
  Unless you have sufficient room on your working WordStar program 
  disk for the files TW.COM, SPELL.COM, MARKFIX.COM, REVIEW.COM and 
  MAINDICT.CMP you will not be able to run a spell check from the 
  Opening Menu.  You will need to exit WordStar and replace the 
  working WordStar program disk with the dictionary disk you created 
  during installation.  This disk should contain the files listed 
  above.  Make sure the disk in drive B has the file you want to 
  spell-check.
  
  Follow the directions for running a spell check in The WORD Plus 
  manual. 
  

UPGRADING FROM A PREVIOUS RELEASE
---------------------------------

  This release of WordStar contains many new features and commands.
  See the "What's New" booklet for a complete list.  The following
  changes came in too late to be included in the documentation.

Printer Patches

  Previous versions of WordStar treat most dot matrix printers 
  and other non-daisy wheel printers as a DRAFT printer with a 
  few patchable items. Because of this, many users have used 
  these patches to be able to use certain features of their 
  printers. Sometimes the patches have been quite extensive, and 
  some users have many files that count on them.

  The printer drivers of WordStar Release 4, on the other hand, 
  are very powerful. Almost every driver recognizes all the print 
  controls and all the dot commands. In fact, if a document is 
  written to be printed on one kind of printer, it is likely that 
  it will also print fine on some other printer.

  However, if you want to use your existing files with WordStar 
  4, and those files rely on the user area being patched in a 
  special way, you can probably do so by moving the patches into 
  WordStar 4, and using the CUSTOM or SIMPLE printer driver.

  On the INSTALL disk is a program called MOVEPRN.COM that 
  copies the printer driver portion of the previous release's 
  user area into files that can be installed into Release 4 with 
  the "auto patcher" feature.

  Copy the program MOVEPRN.COM onto the disk containing the 
  WS.COM file for the previous version. Type 

     MOVEPRN WS.COM FILE1.PAT FILE2.PAT

  MOVEPRN extracts the proper portions of the user area and 
  writes them into two files that may then be used with the "auto 
  patcher" feature of WSCHANGE.

  FILE1.PAT is to be used with the general patching menu 
  (Choose E "Patching" on the WSCHANGE Main Menu, then A "Auto 
  Patcher").  FILE2.PAT should be used to install strings first 
  into the SIMPLE driver, and then into the CUSTOM driver (choose
  B "Printer" on the WSCHANGE Main Menu, then B "Printer driver
  library", D "Change printer driver data" and D "Driver auto
  patcher").

  Test print your document first with the SIMPLE driver, and then 
  with the CUSTOM driver to see which one produces the most 
  satisfactory results.
  
  Also read Appendix C for more information on using the Auto 
  Patcher.


Hanging Indents

  For WordStar Professional Release 4, MailMerge reformats indented 
  text created with ^OG to the current margins.  If you want the text 
  to remain  indented, use embedded ruler lines or the .RM, .LM, 
  and .PM commands.  See the "Reference Guide" for more information.

  Pressing ^OG to wrap back to the first tab on the ruler line after 
  having reached the last tab works the same way it did in previous 
  versions of WordStar, contrary to what is stated in the manual.


TERMINALS
---------

  WordStar comes installed for an "idealized" special terminal. 
  WINSTALL and WSCHANGE allow you to install many terminals by 
  name, thus allowing WordStar to take advantage of the special 
  features that the terminal might support, such as underlining 
  or the function keys.
    
  Use either WINSTALL or WSCHANGE to pick your specific terminal 
  or computer screen from the Monitor menu.  If your terminal 
  isn't on the menu, it probably emulates one of those that is 
  there.   Look in your terminal documentation to find out.

  After you install WordStar for the proper terminal, run 
  WordStar and open the file PRINT.TST to see  which attributes 
  (such as bold and underline) work on your screen.  
  WordStar will highlight the following in some way...

     Bold           (^PB)
     Underline      (^PS)
     Strike-out     (^PX)
     Subscript      (^PV)
     Superscript    (^PT)
     Doublestrike   (^PD)
     Italics        (^PY)
     Blocks         (^KB, ^KK)
     Error messages

  Most of the time, normal text will be shown in dim intensity, 
  and highlighted text will be shown in bright intensity.  You 
  may have to use a brightness and/or contrast knob to adjust  
  your screen the first time you use WordStar this way.

  If your dim intensity is too dim to see well, and you can't  
  adjust it, you can change the BRITE flag to ON using WSCHANGE.  
  This will invert bright and dim in your text, so that regular 
  text is displayed bright, and highlighted text will be 
  displayed as dim. However, text in the menus is not affected.


DISPLAY PROBLEMS WITH TERMINALS
-------------------------------

  Once you have installed WordStar for the proper terminal, you 
  may still experience display problems.

  If text from the previous screen remains after WordStar 
  displays a new screenful of text, the most likely cause is 
  cursor wrap.  Basically, WordStar must know what happens to the 
  cursor when a character is displayed at the rightmost position 
  of the screen.  It can either remain at the right edge, or it 
  can wrap to the beginning of  the next  line.  The WRAP flag in 
  WordStar must be set either on or off to correspond to the 
  way the terminal works.  (It is generally set for the 
  terminal's factory default, but the default can usually be 
  changed using the terminal's setup mode.)

  Another possible cause for display problems is your terminal's 
  incomplete emulation of some other terminal.  The most 
  common differences are...

     Line insert (LININS), line delete (LINDEL),
     Erase to end of screen (ERAEOS),
     Erase to end of line (ERAEOL),
     And, erase screen (ERASCR).

  Look in the manual for your terminal and use WSCHANGE to see  
  if the control sequences match.


PRINTERS
--------

WHAT'S IN THIS SECTION

  This section contains the following information:

  Choosing a Printer
  Setting Up Your Printer
  Printer Drivers
  Proportional Printing
  Laser Printers
  Information on Specific Printers

CHOOSING A PRINTER

  WordStar is ready to work with over 100 printers. The printer you
  choose during installation becomes your default printer. However, 
  when you print a document, you can choose any other printer. To 
  choose a default printer, follow these steps:

  1. Look at the Printer Information brochure that came in your 
     package.  The first chart shows the printers listed on the 
     Printer Selection Menus. If your printer is on the menu, 
     simply choose it during installation.

  2. If your printer isn't listed on the menu, it may work like a
     printer that is. Refer to the second chart in the Printer
     Information brochure for a list of printers that work like
     printers on the menu. When WordStar asks you to choose a
     printer, choose the printer that works like yours.

  3. If neither chart lists your printer, choose Typewriter Printer
     (if your printer can backspace) or Draft Printer (if it can't).
     These choices may not take advantage of all your printer's
     features, but they will work with almost any printer.
 
  Note:  If you choose Draft or Typewriter, you can modify custom
  print controls and printer initialization.

  If you want to make more modifications to take advantage of your
  printer's feature, choose the Custom or Simple drivers, then use 
  the WS Printer Patches section of WSCHANGE to tell WordStar the 
  codes for your printer. Refer to your printer manual for these 
  codes. Some printers work better with the Custom driver and some
  with the Simple driver. Try using both and see which works better 
  with your printer. See the "Reference Guide" for more information. 

SETTING UP YOUR PRINTER

Choosing a Printer Port

  Each printer is connected to a printer port at the back of
  the computer. WordStar looks for printers on the LST: port.
  If your printer is connected to a different port, use
  WSCHANGE to tell WordStar the correct port.

Testing Your Printer Connection

  At the operating system prompt, type "PIP LST:=READ.ME." This 
  file should be printed by your printer. If it is not, your printer 
  may be connected to a different port. See your computer reference 
  manual, and the section on the STAT command in your CP/M 
  reference manual for more information.


PRINTER DRIVERS

  The WSPRINT.OVR file on the Printers disk contains a printer 
  driver for each printer on the Printer Selection Menu. The printer 
  driver for a printer contains all the codes WordStar needs to work 
  with that printer.  
  
  Each printer driver has a short name. If you choose a printer when
  you print a document, you see the names of the printer drivers, not
  the names of the printers.

PROPORTIONAL PRINTING

  WordStar supports proportional printing on a number of printers.
  To turn on proportional printing, either install WordStar to
  default to proportional printing, or place a ".PS on" command
  in your document. At print time, WordStar selects the
  appropriate proportional font based on the character width
  (.CW) currently in effect.

  The specific printer descriptions later in this section show
  recommended character widths for proportional typefaces.
  These widths are for a normal mix of upper- and lowercase
  letters. If you have many words or phrases all in uppercase
  or if you want your text less densely printed, choose a larger
  character width.

  While WordStar mostly sets character widths based on the
  proportional-width table in the driver, on the more advanced
  daisy wheel printers, WordStar uses the printer's proportional-
  spacing mode. WordStar determines how much white space is needed
  to right-justify the line based on its own proportional width 
  tables. If the table values don't match the wheel installed,
  WordStar won't be able to justify the line correctly.

  WordStar sends standard ASCII characters; if a proportional wheel 
  uses a different spoke mapping, set up the printer to handle this.

LASER PRINTERS

  WordStar supports laser printer features such as font changes
  and proportional spacing.

  WordStar supports several laser printers: the Canon LPB-8 A1 & A2;
  the Hewlett-Packard LaserJet, LaserJet+, and LaserJet 500+; 
  and the Ricoh LP4080. Refer to the "Specific Printer
  Information" section of this file for information on these 
  printers. General notes about using laser printers are given below.

Paper Size and Margins

  Laser printers come with preset page margins. You need to 
  compensate for these margins by changing page length in your 
  WordStar documents. The chart below shows the recommended 
  settings for 8 1/2 X 11 inch paper for both portrait and landscape 
  orientations. These settings allow 55 lines of text for portrait 
  orientation and 40 lines of text for landscape orientation (at 6 
  lines per inch). They also allow for a footer of up to 3 lines 
  and a one-line header. If you use multiple-line headers, adjust 
  the top margin accordingly.

                 Dot      Default  Portrait     Landscape
  Setting        Command  Value    Orientation  Orientation
  -------        -------  -------  -----------  -----------
  page length     .PL       66         62           47
  top margin      .MT        3          2            2
  bottom margin   .MB        8          5            5
  header margin   .HM        2          1            1
  footer margin   .FM        2          2            2

  If the laser printer is your primary printer, you can use WSCHANGE
  to make these settings the defaults.

  Because laser printers leave small margins at the left and right
  sides of the page, you may want to use a smaller page offset 
  setting (the default is .PO 8).

Form Feeds

  When you print with a laser printer, answer Y for yes to the "Use
  form feeds (Y/N)?" prompt at print time. (The default is NO.) If
  the laser printer is your primary printer, you can use WSCHANGE to
  change the default to yes.

WordStar Commands for Font Selection

  The WordStar dot commands and print control commands listed below
  determine the fonts used for printing a document.

  .PR  .PR OR=L selects landscape orientation; .PR OR=P (or just
       .PR OR) selects portrait orientation (the default). If
       either of these commands appears after the first printing
       line on a page, the orientation will not change until the
       following page. 

  .PS  .PS ON selects proportionally spaced characters; .PS OFF
       (the default) selects fixed-spaced characters.

  .CW  The character-width setting (.CW followed by the width in
       120ths of an inch) determines the character pitch and font
       selected for fixed-width printing. For proportional fonts, it
       determines the point size and proportional-width table 
       selected.

  .LQ  .LQ ON selects near letter quality print (if supported by
       your printer).  LQ OFF selects draft quality print.  Default
       is ON.

  ^PY  The italic print control toggles between normal and italic
       characters when the appropriate italic font is available.

  ^PB  The boldface print control toggles between normal and bold
       characters when the appropriate bold font is available.

  ^PD  The double strike print control used with the laser printers
       toggles overprinting with a horizontal offset of 1/120"
       between the two character images. This allows a bold effect
       where no bold font is available. 

  ^PA  ^PA turns alternate pitch on. Use .CW to assign different
       character widths to normal pitch (see ^PN below) and alternate
       pitch so that each pitch accesses a different font. You can 
       then change fonts by switching between the two pitches. This 
       is the only way to use two fonts on the same line. 
       (See "Character width" and "Pitch" in the "Reference Guide.")

  ^PN  ^PN turns normal pitch on. You can use it with ^PA as
       described above.

  ^P@  When working with columns, if you use alternate and normal
       pitch for two fonts, or if you use proportional spacing, you
       may need to use ^P@ to make sure the columns line up.
       Remember that the column position set with ^P@ is determined
       by the normal pitch character width. (See "Columns" and
       "Proportional spacing" in the "Reference Guide." 

INFORMATION ON SPECIFIC PRINTERS

  This section describes the capabilities of each printer listed on 
  the Printer Selection Menu. The printers are listed in alphabetical 
  order (except for the generic printers such as "Draft," 
  "Typewriter," "Custom," "Simple," and the various print-to-disk 
  options, which are listed first).  

  There is a chart for each printer explaining how features work and 
  listing any special notes about the printer.  Each printer is 
  described in the following format:

PRINTER NAME ----- Driver: (short name)

 ^PY    Effect of italics/ribbon color print control
 ^PT/V  Subscript/superscript information
 .CW    Information on available character widths and fonts.  The
        chart shows the .CW, .LQ, and .PS settings required to use 
        different fonts.

        .LQ OFF   .LQ ON    .PS ON                      Font Name
        -------   ------    ------                      ---------
        .cw val   .cw val   recommended value (range)   font 1
        .cw val   .cw val   recommended value (range)   font 2

 .UL    Continuous-underline information (if restrictions)
 .UJ    Microspace-justification information (if restrictions)

        N/A means a command has no effect on this printer.

 NOTES  Switch settings, special features, anomalies.

DRAFT PRINTER (nonbackspacing) ----- Driver: DRAFT

 ^PD    Overprints the line twice
 ^PB    Overprints the line three times
 ^PS    Overprints the underscore character in a separate pass
 ^PT/V  Prints super/subscripts with a full line between
        super/subscript and text
 .LH    Sets line height only in multiples of full lines
 .CW    N/A
 .PS    N/A
 .LQ    N/A
 .UJ    N/A

 NOTES  This driver works with any printer that doesn't automatically
 perform a line feed when it receives a carriage return command.  All
 overprinting is done by returning the carriage and passing over the
 line again.

TYPEWRITER PRINTER (backspacing) ----- Driver: TYPEWR

 ^PD    Backspaces and overprints each character twice
 ^PB    Backspaces and overprints each character three times
 ^PS    Backspaces and overprints the underscore character
 ^PT/V  Prints super/subscripts with a full line between
        super/subscript and text
 .LH    Sets line height only in multiples of full lines
 .CW    N/A
 .PS    N/A
 .LQ    N/A
 .UJ    N/A

 NOTES  This driver works with any printer that doesn't automatically
 perform a line feed when a it receives a carriage return command,
 and responds to a backspace character.  Overprinting is done by
 backspacing.

AUTO LINE FEED PRINTER (backspacing) ----- Driver: AUTOLF

 ^PD    Backspaces and overprints each character twice
 ^PB    Backspaces and overprints each character three times
 ^PS    Backspaces and overprints the underscore character
 ^PT/V  Prints super/subscripts with a full line between
        super/subscript and text
 .LH    Sets line height only in multiples of full lines
 .CW    N/A
 .PS    N/A
 .LQ    N/A
 .UJ    N/A

 NOTES  This driver works with any printer that automatically
 performs a line feed when it receives a carriage return character,
 and responds to a backspace command.  Overprinting is done by
 backspacing.

SIMPLE CUSTOMIZABLE PRINTERS ----- Driver: SIMPLE

 All print controls cause control strings (on and off) in
 the user area to be sent to the printer.  These strings
 are used by both the SIMPLE and CUSTOM drivers.  They can
 be installed with the WSCHANGE program.

 .LQ    Controlled by user area strings
 .PS    Controlled by user area strings
 .CW    N/A
 .UJ    N/A
 .LH    N/A

 NOTES  This printer driver prints the line in one pass, sending
 control strings from the user area to select print enhancements.

CUSTOMIZABLE PRINTERS ----- Driver: CUSTOM

 All print controls cause control strings (on and off) in
 the user area to be sent to the printer.  These strings
 are used by both the SIMPLE and CUSTOM drivers.  They can
 be installed with the WSCHANGE program.

 .LQ    ON/OFF controlled by user area strings
 .PS    ON/OFF controlled by user area strings
 .LH    Sets line height only in multiples of full lines
 .UJ    N/A
 .CW    N/A

 NOTES  This driver prints the line in multiple passes, sending
 control strings from the user area to select print enhancements.

PREVIEW TO DISK ----- Driver: PRVIEW

 This driver prints documents to the PREVIEW.WS file to allow
 you to preview the format and appearance of a document before
 printing. Headers, footers, and pagination are shown correctly
 and print controls remain in the file to display onscreen
 attributes.  Dot commands are not printed.

PRINT TO DISK WITHOUT PRINT CONTROLS ----- Driver: ASCII

 This driver prints to the ASCII.WS file, stripping headers and
 footers, high bits, and print controls.

PRINT TO DISK WITHOUT HEADERS AND FOOTERS ----- Driver: XTRACT

 This driver prints to the XTRACT.WS disk file, stripping headers
 and footers, but preserving high bits and print controls.

ANADEX 9500A, 9500B ----- Driver: 9500

 ^PY    N/A
 ^PT/V  Even superscript roll

 .CW    .CW  Font name
        ---  ---------
         9   13.3 cpi
        10   12   cpi
        12   10   cpi
        18    6.7 cpi
        20    6   cpi
        24    5   cpi

 .LH    1/24" resolution, use even values
 .UJ    This printer has no incremental horizontal positioning
 .PS    N/A
 .LQ    N/A

ANADEX 9501B, INTEQ 5100B ----- Driver: 9501B

 ^PY    N/A
 ^PT/V  Even superscript roll

 .CW    .CW  Font name
        ---  ---------
         7   16.7 cpi
         8   15   cpi
        10   12.5 cpi
        12   10   cpi
        14    8.3 cpi
        16    7.5 cpi
        20    6.2 cpi
        24    5   cpi

 .LH    1/24" resolution, use even values
 .UJ    This printer has no incremental horizontal positioning
 .PS    N/A
 .LQ    N/A

C. ITOH STARWRITER 1550 AND 8510 ----- Driver: C1550

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification

C. ITOH F10 STARWRITER ----- Driver: QUME

 See Diablo 630, 1610, 1620 Daisy Wheel.
 
 Note:  Proportional printing was tested with a Theme 10 wheel.

CANON LBP-8A1 AND LBP-8A2 LASER PRINTER ----- Driver: LBP8

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll
         .PS .PS
 .CW     OFF  ON           Font Name
         ---  --           ---------
          6   -            20 cpi
          8   -            15 cpi
          9   -            13.3 cpi
         10   -            12 cpi (elite)
         12   -            10 cpi
         20   -            6 cpi
         24   -            5 cpi
         16   -            7.5 cpi
         -     7 (0-8)     Garland 8 point
         -    10 (9-11)    Garland 12 point
         -    14 (12-17)   Expanded 8 point
         -    20 (18-30)   Expanded 12 point

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended
 .PR OR "=Landscape" or "=Portrait" to select orientation

 NOTES  Answer yes to the "Use form feeds" prompt. This driver is 
 configured to select all the built-in fonts in the LBP8, as well 
 as fixed pitch cartridges and the Garland PS cartridge.  Other 
 proportional cartridges require modifying the proportional spacing 
 tables with WSCHANGE.  For more information on laser printers, see 
 the "Laser Printers" section above.

CITIZEN MSP ----- Driver: CITMSP

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW    Font Name
        ---    ---------
         7     compressed
        10     elite
        12     pica
        14     expanded compressed
        20     expanded elite
        24     expanded pica

 .LH    Use even values.  Driver operates at 2/48 resolution.
 .PS    N/A
 .UJ    Microjustification slows printing.  Continuous underlining
        suppresses microjustification.


DATAPRODUCTS PAPER TIGER SPG-8050 & SPG-8070 ----- Driver: SP8050

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, prints full-size
        .LQ  .LQ  .PS
 .CW     ON  OFF   ON          Font name
        ---  ---  ---          ---------
         7    7     5 (0-6)    condensed
        10   10     8 (7-8)    elite
        12   12    10 (9-13)   pica
        14   14     -          expanded condensed   
        20   20    16 (14-17)  expanded elite  
        24   24    20 (18-30)  expanded pica

DIABLO 630, 1610, 1620 DAISY WHEEL ----- Driver: DIABLO

 ^PY    Selects red/black ribbon color
 ^PT/V  Prints super/subscripts in separate pass with specified roll
 .CW    Supports any value from 0 to 30.  Usual fixed pitch values 
        are 8 (15 cpi), 10 (12 cpi), and 12 (10 cpi).
 .BP    ON selects bidirectional printing; OFF selects left-to-right
        printing
 .LQ    N/A
 .UL    Continuous underlining does not suppresses microspace
        justification.  Continuous underlining may be irregular.
 .PS    ON selects proportional spacing; OFF selects fixed pitch
        spacing.  If a proportional print wheel has a non-standard
        spoke pattern, configure the printer to translate spoke
        position into the appropriate character.  This driver
        explicitly positions each character when proportional spacing
        is selected.

 NOTES  The proportional spacing tables are set up for a Diablo
 metal 96 character BOLD PS wheel.

DIABLO 630 DAISY WHEEL WITH WP OPTIONS ----- Driver: 630WP

 ^PY    Selects red/black ribbon color
 ^PT/V  Prints super/subscripts in separate pass with specified roll
 .CW    Supports any value from 0 to 30.  Usual fixed pitch values 
        are 8 (15 cpi), 10 (12 cpi), and 12 (10 cpi).
 .LQ    N/A
 .UL    Continuous underlining does not affect microspace justifi-
        cation
 .PS    ON selects proportional spacing; OFF selects fixed pitch
        spacing.  If a proportional print wheel has a non-standard
        spoke pattern, configure the printer to translate spoke
        position into the appropriate character.  This driver sends
        codes to the printer to turn proportional spacing on and off,
        and the printer controls character to character spacing.

 NOTES  The proportional spacing tables are set up for a Diablo
 metal 96 character BOLD PS wheel.

DIABLO 630 DAISY WHEEL, EXTENDED CHARACTER SET ----- Driver: 630ECS

 ^PY    N/A
 ^PT/V  Prints super/subscripts in separate pass with specified roll
 .CW    Supports any value from 0 to 30.  Usual fixed pitch values 
        are 8 (15 cpi), 10 (12 cpi), and 12 (10 cpi).
 .LQ    N/A
 .UL    Continuous underlining does not affect microspace justifi-
        cation
 .PS    ON selects proportional spacing; OFF selects fixed pitch
        spacing.  If a proportional print wheel has a non-standard
        spoke pattern, configure the printer to translate spoke
        position into the appropriate character.  This driver sends
        codes to the printer to turn proportional spacing on and off,
        and the printer controls character to character spacing.

 NOTES  The proportional spacing tables have been set up for a Diablo
 metal 96 character BOLD PS wheel.

DIABLO C150 & C200 COLOR JET PRINTERS ----- Driver: C150

 ^PY    Selects red/black ink
 .CW    10 characters per inch only
 .LH    1/30" resolution
 .PS    N/A
 .LQ    N/A

EPSON FX-80 AND FX-100 ----- Driver: FX80

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

EPSON FX-85, FX-185 AND FX-286 ----- Driver: FX85

 ^PY    Selects draft quality italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         6   -    -            compressed elite
         7   -    -            compressed
        10   -    -            elite
        12   12   11 (10-13)   courier
        14   -    -            expanded compressed
        20   -    -            expanded elite
        24   24   22 (20-30)   expanded courier

 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.
        .UJ must be on for proportional text to be right-justified.

EPSON LQ-800 AND LQ-1000 ----- Driver: LQ800

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON     Font Name
        ---  ---  ------     ---------
        -    -    -          compressed script
         6    6   -          compressed elite
         7    7    6 (0-7)   compressed
         8        -          subscript 15 cpi
        10   10   -          elite
        12   12   10 (8-16)  pica
        14   14   -          expanded compressed
        16        -          expanded script
        20   20   -          expanded elite
        24   24   -          expanded courier

EPSON LQ-1500, VERSION 2.0 ----- Driver: LQ1500

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        10   10   -            elite
        -    -     8 (1-9)     subscript 15 cpi
        12   12   11 (10-13)   courier
        14   -    -            expanded compressed
        -    -    15 (14-18)   expanded script
        20   20   -            expanded elite
        24   24   20 (19-30)   expanded courier

 .UL    Continuous underlining suppresses microspace justification.
        In proportional fonts, continuous underlining may appear
        broken between words.

 NOTES  If you have an older LQ-1500 (firmware version 1.8), your
 printer will have horizontal position registration problems.  For
 best results, contact your printer dealer about a ROM upgrade.

EPSON LX-80 - Driver: LX80

 ^PY    Selects draft mode italics
 ^PT/V  Prints half height if .SR 0, else full height with roll

        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7   -    compressed
        10   -    elite
        12   12   courier
        14   -    expanded compressed
        20   -    expanded elite
        24   24   expanded courier

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

EPSON MX-80 AND MX-100 WITH GRAFTRAX+
EPSON MX-80 III AND MX-100 III ----- Driver: MX80

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        12   pica
        14   expanded compressed
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

 NOTES  Older MX-80 and MX-100 printers don't have graphics mode (for
 fine horizontal spacing), variable line height setting, printer
 controlled underlining, or printer controlled super/subscripts.  If
 you have one of these printers, use the DRAFT driver, or adapt the
 CUSTOM or SIMPLE driver to your needs.

EPSON RX-80 AND RX-100 ----- Driver: RX80

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

HEWLETT-PACKARD LASERJET PRINTERS

 The following information applies to the LaserJet, the LaserJet+,
 and the LaserJet 500+.  For general information on laser printers,
 see the "Laser Printers" section above.

The LaserJet Fonts

 The LaserJet has three different types of fonts:

 - The "internal" fonts that came with the printer
 - Plug-in cartridges
 - Soft fonts that must be downloaded through your computer.
   (Only the LaserJet+ and LaserJet 500+ can use downloaded fonts.)

 The fonts available in your LaserJet depend on which cartridge
 you have installed and which fonts you have downloaded.

Font Installation

 Internal Fonts:

 The fonts that came with your printer are already in memory and
 ready to use. Different LaserJet models come with different sets
 of internal fonts.

 Cartridges:

 Cartridges containing a variety of character fonts can be
 inserted into any LaserJet model. See your printer manual for
 instructions.

 The font selection guidelines in the sections below contain
 information about specific cartridges. The letter that identifies
 your cartridge is on the front label, directly following the
 number 92286.  For example, the Y cartridge is labeled 92286Y.

 Soft fonts:

 Soft, or downloadable, fonts are supplied on disk.  These fonts 
 are not explicitly supported by WordStar.

LaserJet Font Selection

 Each LaserJet font has several characteristics associated with
 it. When a printer driver specifies font characteristics to the
 LaserJet, the LaserJet searches its available fonts for the best
 match to the characteristics requested. The following table
 describes these characteristics, in the order in which the
 LaserJet evaluates them when selecting a font.

 Characteristic                         WordStar Control
 --------------                         -----------------
 * Orientation (portrait or landscape)  .PR OR=P/L
 * Symbol Set (Roman-8, USASCII,        Printer driver
   Line Draw, etc.)
 * Proportional or fixed spacing        .PS ON/OFF
 * Print pitch (fixed-width fonts)      .CW
 * Character height (point size)        .CW
 * Character style (upright or italic)  ^PY
 * Stroke weight (light, medium, bold)  ^PB

 Note that symbol set is high in the list of characteristics:
 make sure that the driver you select is compatible with the symbol 
 set of your cartridge or downloaded fonts. The symbol sets used by 
 each driver are listed in the table in the next section. For example, 
 if your cartridge has the USASCII Symbol Set, you can't use the 
 HPLJ:U driver because it uses only the Roman-8 Symbol Set.

LaserJet Printer Drivers

 WordStar provides two printer drivers for use with different
 LaserJet font cartridges. Each of these drivers
 lets you print with several of the available fonts. You can 
 use any of these drivers with the LaserJet, LaserJet+, or
 LaserJet 500+, depending on the cartridge.
 Refer to the table below to see which driver works
 best for you.

 The table lists the following information for each driver:

 o  The symbol sets used for fixed and proportional spacing

    These must correspond to the symbol sets on the installed
    fonts you want to use. The "Default" symbol set refers to the
    one the LaserJet defaults to.

 o  The proportional-spacing tables used by the driver

    These tables are part of the LaserJet's method of proportional
    spacing. The tables determine the width of each character in a 
    proportionally spaced font. The fonts corresponding to these 
    tables are used if available. If the corresponding font is not 
    installed, the table is still used, and the closest available 
    font is used. This may cause the spacing to appear too tight or 
    too loose. In this column, the number is the point size, R stands 
    for regular, B stands for bold, and I stands for italics (the 
    LaserJet has separate tables for each of these).

 o  The font cartridges that work best with
    the symbol sets and tables used by the driver

    The cartridges listed are the only ones directly
    supported for use with WordStar. If your cartridge is not 
    listed, you may still be able to use it. Look at
    the font information below and try the most compatible driver. 
    You may need to try different dot command settings or another 
    driver. The HPLJET is the most "general purpose" driver, so if 
    you're not sure which driver to use, try it first.

         Fixed-width  Proportional  Proportional   Downloaded
 Driver  Symbol Set   Symbol Set    Tables         Fonts/Cartridges
 ------  -----------  ------------  -------------  ----------------

 HPLJET  Default      Default       TmsRmn 8R,     F, P, most fixed
                                    10R,10B,10I
                                    Helv 14B

 HPLJ:B  Default      USASCII       TmsRmn 8R,     B
                                    10R,10B,10I
                                    Helv 14B

 HPLJ:U  Roman-8,     Roman-8       Helv 6R,8R,    U, V
         Line Draw                  10R,12R,14R

 HPLJ:Y  PCSET1       USASCII       TmsRmn         Y, AC
         PCSET2                     6,8,10,12,14
                                    (all in R,B,I)
                                    18B,24B,30B

 HPL:AD  Roman-8,     Roman-8       TmsRmn         AD
         Line Draw                  6,8,10,12,14
                                    (all in R,B,I)
                                    18B,24B,30B

 The printer driver charts below show the actual fonts that print
 with each printer driver and the recommended font cartridges. 
 The charts show the fonts used for both fixed
 and proportional spacing and for different character width (.CW)
 settings.

 The recommended .CW settings are shown first. The settings in
 parentheses select the same font, but the spacing of characters
 within a line may appear tighter or looser.

 After the name of each font, the charts note whether regular (R),
 bold (B), and italic (I) fonts are available. If a bold font is
 not available, you can use the ^PD (double strike) command to get
 a boldface effect.

 The last column shows whether you can print in landscape (chosen
 in WordStar with .PR OR=L) as well as portrait orientation.

 To use a particular font, choose the settings listed.  For example,
 to use the Times Roman 8 font with the HPLJET printer driver, insert
 the F cartridge, turn .PS on and set character width to .CW 7.

HP LASERJET, LASERJET+ (F cartridge and others) ----- Driver: HPLJET

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll

  Cartridge/
  Soft font .PS  .CW        Font/Point Size   R B I  Landscape
  --------- ---  --------   ---------------   - - -  ---------
     F      on    7 (0-7)   Times Roman 8     x
                  9 (8-11)  Times Roman 10    x x x
                 13 (12-30) Helvetica 14        x
            off   7 (0-11)  Line Printer 8.5  x
                 12 (12-30) Courier 12        x         x
     P      on    9 (0-30)  Times Roman 10    x x x     x
            off   7 (0-11)  Line Printer 8.5  x
                 12 (12-30) Courier 12        x         x (0-30)

        The following fixed pitch fonts may be available depending
        on your cartridge. (Note that these are measure by pitch, 
        not by point size.):

          .CW  Font Name
          ---  ---------
           7   16.7 pitch
          10   12 pitch
          12   10 pitch
          15   8.1 pitch
          18   6.5 pitch
          21   5.8 pitch
          27   4.5 pitch

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended.
        Too large a value will cause text to be lost at page bottom.
 .PR OR "=Landscape" or "=Portrait" to select orientation.

 NOTES  Answer yes to the "Use form feeds" prompt.  This driver has
 proportional spacing tables for all fonts in the F and P cartridges.
 It should also work with many fixed width cartridges.
.p

HP LASERJET, LASERJET+ (B cartridge) ----- Driver: HPLJ:B

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll

  Cartridge/
  Soft font .PS  .CW        Font/Point Size   R B I  Landscape
  --------- ---  --------   ---------------   - - -  ---------
     B      on    7 (0-7)   Times Roman 8     x
                  9 (8-11)  Times Roman 10    x x x
                 13 (12-30) Helvetica 14        x
            off   7 (0-11)  Line Printer 8.5* x         x
                 12 (12-30) Courier 12        x         x
        * Line printer 8.5 is not available in portrait mode
          unless the LaserJet+ is used.

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended.
        Too large a value will cause text to be lost at page bottom.
 .PR OR "=Landscape" or "=Portrait" to select orientation.

 NOTES  Answer yes to the "Use form feeds" prompt. This driver has
 proportional spacing tables for all fonts in the B cartridge.
.p

HP LASERJET, LASERJET+ (U and V cartridges) ----- Driver: HPLJ:U

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll

  Cartridge/
  Soft font .PS  .CW        Font/Point Size   R B I  Landscape
  --------- ---  --------   ---------------   - - -  ---------
     U      on    5 (0-5)   Helvetica 6       x
                  7 (6-7)   Helvetica 8       x
                  9 (8-9)   Helvetica 10        x
                 11 (10-11) Helvetica 12        x
                 13 (12-30) Helvetica 14        x
            off   7 (0-11)  Letter Gothic 9.5 x
                 12 (12-30) Courier 12        x        x (0-30)

     V      on    5 (0-5)   Helvetica 6       x     landscape only*
                  7 (6-7)   Helvetica 8       x        "*
                  9 (8-9)   Helvetica 10        x      "*
                 11 (10-11) Helvetica 12        x      "*
                 13 (12-30) Helvetica 14        x      "*
            off   7 (0-11)  Letter Gothic 9.5 x         **
                 12 (12-30) Courier 12        x
         * No proportional font is available in portrait orientation.
        ** With fixed spacing, in portrait orientation, .CW7 (0-11)
           produces Line Printer 8.5 on the LaserJet+ and Courier 12
           on the LaserJet.

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended.
        Too large a value will cause text to be lost at page bottom.
 .PR OR "=Landscape" or "=Portrait" to select orientation.

 NOTES  Answer yes to the "Use form feeds" prompt. This driver has
 proportional spacing tables for all fonts in the U and V cartridges.
.p

HP LASERJET, LASERJET+ (Y cartridge, AC TmsRmn) ----- Driver: HPLJ:Y

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll

  Cartridge/
  Soft font .PS  .CW        Font/Point Size   R B I  Landscape
  --------- ---  --------   ---------------   - - -  ---------
     Y      on   none available
            off   7 (0-11)  Line Printer 8.5  x        x
                 12 (12-30) PC Courier 12     x x x

    AC*     on    5 (0-5)   Times Roman 6     x x x    x
                  7 (6-7)   Times Roman 8     x x x    x
                  9 (8-9)   Times Roman 10    x x x    x
                 11 (10-11) Times Roman 12    x x x    x
                 13 (12-14) Times Roman 14    x x x    x
                 16 (15-18) Times Roman 18      x      x
                 20 (19-24) Times Roman 24      x      x
                 25 (25-30) Times Roman 30      x      x
            off   7 (0-11)  Line Printer 8.5  x        x (0-30)
                 12 (12-30) Courier 12        x
        * Other .CW settings may access additional fonts if a
          cartridge is also installed.

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended.
        Too large a value will cause text to be lost at page bottom.
 .PR OR "=Landscape" or "=Portrait" to select orientation.
 
 NOTES  Answer yes to the "Use form feeds" prompt. This driver is for 
 use with the Y cartridge, which provides an IBM PC compatible symbol
 set.  In addition, this driver has complete proportional spacing 
 tables for the AC set of downloadable TmsRmn fonts.
.p

HP LASERJET, LASERJET+ (AD TmsRmn) ----- Driver: HPL:AD

 ^PY    Selects italics if appropriate font installed
 ^PT/V  Prints full-size characters with roll

  Cartridge/
  Soft font .PS  .CW        Font/Point Size   R B I  Landscape
  --------- ---  --------   ---------------   - - -  ---------
    AD*     on    5 (0-5)   Times Roman 6     x x x    x
                  7 (6-7)   Times Roman 8     x x x    x
                  9 (8-9)   Times Roman 10    x x x    x
                 11 (10-11) Times Roman 12    x x x    x
                 13 (12-14) Times Roman 14    x x x    x
                 16 (15-18) Times Roman 18      x      x
                 20 (19-24) Times Roman 24      x      x
                 25 (25-30) Times Roman 30      x      x
            off   7 (0-11)  Line Printer 8.5  x
                 12 (12-30) Courier 12        x        x (0-30)

        The following fixed pitch fonts may be available depending
        on your cartridge. (Note that these are measure by pitch, 
        not by point size.):

          .CW  Font Name
          ---  ---------
           7   16.7 pitch
          10   12 pitch
          12   10 pitch
          15   8.1 pitch
          18   6.5 pitch
          21   5.8 pitch
          27   4.5 pitch

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended.
        Too large a value will cause text to be lost at page bottom.
 .PR OR "=Landscape" or "=Portrait" to select orientation.
 
 NOTES  Answer yes to the "Use form feeds" prompt. This driver is for
 use with the AD TmsRmn downloaded fonts, and for a ROMAN8 or 
 ROMAN8+LINEDRAW fixed width font cartridge. The driver includes 
 complete proportional spacing tables for the AD set of downloadable 
 TmsRmn fonts.
             
HP THINKJET, IBM mode ----- Driver: HPTJI

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is ON.

 NOTES  This printer does not have a true 10 pitch font, so character
 widths are not exact, and ^P@ does not align exactly with text.  
 Because the printer has an automatic page offset, set the WordStar
 page offset to zero.

IBM COLOR PRINTER 5182 ----- Driver: IBMCLR

 ^PY    Selects red/black ribbon color
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ  .PS
 .CW    OFF   ON   ON         Font Name
        ---  ---  --------    ---------
         7    7    5 (0-6)    compressed
        10   10    8 (7-8)    elite
        12   12   10 (9-13)   pica
        14   14    -          expanded compressed
        20   20   15 (14-16)  expanded elite
        24   24   20 (17-30)  expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    Has same effect as ^PD
 .UL    Underlining may be irregular with microspace justification on
 .UJ    Microspace justification slows printing. Default is OFF.

IBM GRAPHICS PRINTER 5152 ----- Driver: IBMGR

 ^PY    N/A
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        12   pica
        14   expanded compressed
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

IBM PROPRINTER 4201 ----- Driver: IBMPRO

 ^PY    N/A
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7    7   compressed
        10   10   elite
        12   12   pica
        14   14   expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .PS    N/A
 .LQ    Has same effect as ^PD
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

 NOTES  If you have a Proprinter XL, you can use WSCHANGE to patch
 in the extra features.

IBM QUIETWRITER 5201 ----- Driver: IBMQUI

 ^PY    Toggles between A and * font cartridge.  Set character
        width to match cartridge in use.  (A cartridge uses current
        ^PN character width; * cartridge uses ^PA character width.)
 ^PT/V  Prints full-size characters with roll
 .CW    Selects character width.  Character width must correspond
        to the cartridge being used.
 .LQ    N/A
 .PS    ON selects proportional spacing, OFF selects fixed pitch
        spacing

IBM WHEELPRINTER 5216 ----- Driver: IBMWP

 ^PY    N/A
 ^PT/V  Printer determined roll if .SR 0
 .CW    Selects character spacing.  Any value from 0 to 30 is
        supported.   Usual fixed pitch values are 8 (15 characters
        per inch), 10 (12 cpi) and 12 (10 cpi).
 .LQ    N/A
 .UL    Continuous underlining does not affect microjustification
 .PS    ON selects proportional spacing, OFF selects fixed pitch.
        This driver sends codes to the printer to turn proportional
        spacing on and off, and the printer controls character to
        character spacing.

 NOTES  The proportional spacing tables are set up for an IBM
 BOLD PS wheel.

IBM WHEELPRINTER 5223 E ----- Driver: IBMWPE

 ^PY    N/A
 ^PT/V  Printer determined roll if .SR 0
 .CW    Selects character spacing.  Any value from 0 to 30 is
        supported.   Usual fixed pitch values are 8 (15 characters
        per inch), 10 (12 cpi) and 12 (10 cpi).
 .LQ    N/A
 .UL    Continuous underlining does not affect microjustification.  
        Continuous underlining will be somewhat irregular.
 .PS    ON selects proportional spacing, OFF selects fixed pitch.
        This driver will send codes to the printer to turn propor-
        tional spacing on and off, and the printer will control
        character to character spacing.

 NOTES  The proportional spacing tables are set up for an IBM
 BOLD PS wheel.

MANNESMANN TALLY MT-160L ----- Driver: MT160L

 ^PY    N/A
 ^PT/V  Prints full-size characters with specified even roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         6   -    compressed elite
         7   -    compressed
        10   10   elite
        12   12   pica
        14   -    expanded compressed
        20   -    expanded elite
        24   -    expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .UJ    N/A

 NOTES  This printer is not capable of incremental horizontal
 positioning.  As a result, microspace justification is not possible.
 In addition, when changing character widths, characters may not
 align to closer than one full character width.  Also, page offsets
 smaller than a character will not work.

MPI PRINTMATE 99 & 350 ----- Driver: MPI99

 ^PY    N/A
 ^PT/V  Even superscript roll
        .LQ  .LQ  
 .CW    OFF   ON  Font name
        ---  ---  ---------
         7    -   17.1 cpi
        10    -   12   cpi
        12   12   10   cpi
        14    -    8.5 cpi
        20    -    6   cpi
        24   24    5   cpi

 .LH    1/24" resolution, use even values
 .PS    N/A
 .UJ    N/A

NEC PINWRITER P2-3, P2-6, P3-3, P6-6 ----- Driver: NECP2I

 ^PY    N/A
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7   -    compressed
        10   10   elite
        12   12   pica
        14   -    expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 .PS    N/A
 .UL    Continuous underline suppresses microspace justification
 .UJ    Microspace justification slows printing.  Default is OFF.

 NOTES  Page offsets smaller than the character width in effect are
 not supported.  Make sure switch 5 on the printer is off.

NEC PINWRITER P5XL, P6, P7 ----- Driver: NECP5

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         6    6   -            compressed elite
         7    7    6 (0-8)     compressed
         8    8   -            subscript 15 cpi
        10   10   -            elite
        12   12   10 (9-17)    pica
        14   14   -            expanded compressed
        16   16   -            expanded script
        20   20   -            expanded elite
        24   24   20 (18-26)   expanded courier
        30   30   30 (27-30)   triple elite


NEC SPINWRITER 2000R, 3500R
NEC SPINWRITER 2010, 3510, 7710
NEC SPINWRITER 2030, 3530, 7730 ----- Driver: SPINWR

 See Diablo 630, 1610, 1620 Daisy Wheel.

 .BP    N/A

 NOTES  The proportional spacing tables are set up for a NEC BOLD PS
 wheel. Proportional spacing is not supported on the 2010 and 2030.

NEC SPINWRITER 2015, 3515, 7715 ----- Driver: DIABLO

 See Diablo 630, 1610, 1620 Daisy Wheel.

 .BP    N/A

 NOTES  The proportional spacing tables are set up for a NEC BOLD PS
 wheel. This printer does not respond correctly to the phantom blank
 and phantom rubout characters, and may lose horizontal alignment if
 they are included in your document. Proportional spacing is not
 supported on the 2015.

NEC SPINWRITER 2050, 3550, 8850 ----- Driver: SPIN50

 See Diablo 630, 1610, 1620 Daisy Wheel.

 .BP    N/A

 NOTES  The proportional spacing tables are set up for a NEC BOLD PS
 wheel. Proportional spacing is not supported on the 2050.

OKIDATA MICROLINE 84 STEP 2, STANDARD ----- Driver: ML84

 ^PY    N/A
 ^PT/V  Printer controlled if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7    7   compressed
        10   10   elite
        12   12   pica
        14   14   expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 .PS    N/A
 .UJ    In draft mode (.LQ OFF), this printer is not capable of
        microspace justification.  Different character widths may
        not line up correctly.

 NOTES  Page offsets smaller than the character width in effect are
 not supported.

OKIDATA MICROLINE 92 AND 93, STANDARD ----- Driver: ML92

 ^PY    N/A
 ^PT/V  Printer controlled if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7        compressed
        10   10   elite
        12   12   pica
        14        expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 .PS    N/A
 .UJ    In draft mode (.LQ OFF), this printer is not capable of
        microspace justification.  Different character widths may
        not line up correctly.

 NOTES  Page offsets smaller than the character width in effect are
 not supported.

OKIDATA MICROLINE 84, 92, 93, IBM PLUG & PLAY ----- Driver: ML92I

 ^PY    N/A
 ^PT/V  Printer controlled if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7        compressed
        12   12   pica
        14        expanded compressed
        24   24   expanded pica

 .PS    N/A
 .UJ    In draft mode (.LQ OFF), this printer is not capable of
        microspace justification.  Different character widths may
        not line up correctly.

 NOTES  Page offsets smaller than the character width in effect are
 not supported.

OKIDATA MICROLINE 182, STANDARD ----- Driver: ML182
OKIDATA MICROLINE 182, IBM                    ML182I

 ^PY    N/A
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7   -    compressed
        10   10   elite
        12   12   pica
        14   -    expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 NOTES  This printer is not capable of incremental horizontal 
 positioning, so microspace justification is not possible. In
 addition, when changing character widths, characters may not align
 to closer than one full character width. Also, page offsets smaller
 than a character do not work.

OKIDATA MICROLINE 192, STANDARD ----- Driver: ML192
OKIDATA MICROLINE 192, IBM                    ML192I

 ^PY    Selects draft mode italics.  No half height italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON      Font Name
        ---  ---  ------      ---------
         7   -    -           compressed
        10   10    9 (9-10)   elite
        12   12   11 (11-17)  pica
        14   -    -           expanded compressed
        20   20   18 (18-20)  expanded elite
        24   24   22 (21-30)  expanded pica

 NOTES  This printer does not have control strings to select
 proportional and fixed pitch printing. This choice can only be
 made through the printer's own menu functions. For reasonable
 results, make sure that your document and printer are both fixed
 pitch or both proportional.

OKIDATA MICROLINE 292, STANDARD ----- Driver: ML292
OKIDATA MICROLINE 292, IBM                    ML292I

 ^PY    Selects italics.  No half height italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON      Font Name
        ---  ---  ------      ---------
         7    7    7 (6-8)    compressed
        10   10    9 (9-10)   elite
        12   12   11 (11-12)  pica
        14   14   13 (13-17)  expanded compressed
        20   20   18 (18-20)  expanded elite
        24   24   22 (21-30)  expanded pica

 NOTES  This printer does not have control strings to select
 proportional and fixed pitch printing. This choice can only be
 made through the printer's own menu functions. For reasonable
 results, make sure that your document and printer are both fixed
 pitch or both proportional.

OKIDATA PACEMARK 2410, STANDARD ----- Driver: PM2410

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
         7   -    compressed
        10   10   elite
        12   12   pica
        14   -    expanded compressed
        20   20   expanded elite
        24   24   expanded pica

 .UJ    Compressed and expanded compressed characters will not be
        microspace justified.  Also, they may not align perfectly
        with other character widths.

 NOTES  If you have the IBM-compatible printer, do not use this 
 installation.  Instead, choose the IBM Graphics Printer.

PANASONIC KX-P1090 ----- Driver: P1090

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification.

QUME SPRINT SERIES ----- Driver: QUME

 See Diablo 630, 1610, 1620 Daisy Wheel.

 .PS    N/A

 NOTES  Make sure you use the appropriate switch settings for your
 interface module.  Set the switches on the module accordingly:
   IBM Centronics module:  1, 2, 8, 9 ON.  All others OFF.
   RS-232-C module:        1, 2 ON.  All others OFF.

QUME SPRINT WITH WP OPTION ----- Driver: QUMEWP

 See Diablo 630, 1610, 1620 Daisy Wheel.

 .PS    N/A

RICOH LP4080R LASER PRINTER ----- Driver: LP4080

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll
        .PS  .PS
 .CW    OFF   ON         Font Name
        ---  ---         ---------
         8   -           15 cpi
        10   -           12 cpi elite
        12   -           10 cpi courier
        -    11 (0-30)   proportional

 .LQ    N/A
 .PL    For 11 inch paper, a value of 62 is recommended
 .PR OR "=Landscape" or "=Portrait" to select orientation

 NOTES  Answer yes to the "Use form feeds" prompt. This driver is 
 configured to select all the built in fonts in the LP4080R, in both
 portrait and landscape mode.  For more information on laser printers,
 see the "Laser Printers" section above.

SILVER REED EXP-550/500 DAISY WHEEL ----- Driver: SR550

 See Diablo 630, 1610, 1620 Daisy Wheel.

 NOTES  Proportional spacing tables (Model 500 does not support 
 proportional printing) are set up for a Silver Reed PS wheel.  
 You need to change the switch settings for proportional
 fonts.  Set the SW-1 switches accordingly: 
   For proportional fonts:     1, 2 ON, 3-6 OFF
   For nonproportional fonts:  All OFF.

STAR MICRONICS GEMINI 10X AND 15X ----- Driver: GEM10X

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll

 .CW    .CW  Font Name
        ---  ---------
         7   compressed
        10   elite
        12   pica
        14   expanded compressed
        20   expanded elite
        24   expanded pica

 .LH    Use even values.  Driver operates at 2/48" resolution.
 .LQ    N/A
 .PS    N/A
 .UL    Continuous underlining suppresses microspace justification
 .UJ    Microspace justification slows printing. Default is OFF.

STAR MICRONICS NX-10 ----- Driver: NX10

 ^PY    Selects draft quality italics
 ^PT/V  Prints half-size if .SR 0; otherwise full-size with roll
        .LQ  .LQ  .PS
 .CW    OFF   ON   ON          Font Name
        ---  ---  ---          ---------
         6   -     4 (0-5)     compressed elite
         7   -     7 (6-7)     compressed
        10   -     9 (8-9)     elite
        12   12   11 (10-12)   pica
        14   -    -            expanded compressed
        20   -    -            expanded elite
        24   24   -            expanded pica

 .UL    Continuous underlining suppresses microjustification
 .UJ    Microjustification slows printing

STAR MICRONICS SG10  ---- Driver: SG10
STAR MICRONICS SG10I ---- Driver: SG10I

 ^PY    Selects draft mode italics
 ^PT/V  Prints full size characters with roll

        .LQ  .LQ  
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        10   -    10 (9-12)    elite
        12   12   -            pica
        14   -    -            expanded compressed
        20   -    20 (18-24)   expanded elite
        24   24   -            expanded pica

 .UL    Continuous underlining suppresses microjustification
 .UJ    Microjustification slows printing
 .PS	Draft quality proportional

  NOTE:  Because of printer firmware limitations, combinations of
  print enhancements may cause poor printed output.
  
TANDY DMP-130 MATRIX PRINTER ----- Driver: DMP13

 ^PY    Selects italics
 ^PT/V  Prints half-size characters (17 cpi, or 8.5 cpi for 
        expanded fonts)
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        -    10   -            elite
        12   12   11 (11-13)   pica
        14   -    -            expanded compressed
        -    20   -            expanded elite
        24   24   22 (21-30)   expanded pica

 NOTES  Printer must be in Tandy mode.  

TANDY DMP-2100P MATRIX PRINTER ----- Driver: D2100P

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        -    10    9 (9-10)    elite
        12   12   11 (11-13)   pica
        14   -    -            expanded compressed
        -    20   18 (18-20)   expanded elite
        24   24   22 (21-30)   expanded pica

 NOTES  Printer must be in Tandy mode.  

TANDY DMP-2110 MATRIX PRINTER ----- Driver: D2110

 ^PY    Selects italics
 ^PT/V  Prints half-size if .SR 0; otherwise, full-size with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        -    10    9 (9-10)    elite
        12   12   11 (11-13)   pica
        14   -    -            expanded compressed
        -    20   18 (18-20)   expanded elite
        24   24   22 (21-30)   expanded pica

 NOTES  Printer must be in Tandy mode.  

TANDY DWP-230 DAISY WHEEL ----- Driver: DWP230
TANDY DWP-520 DAISY WHEEL ----- Driver: DWP520

 ^PY    N/A
 ^PT/V  Prints super/subscripts in separate pass with specified roll
 .CW    Supports any value from 0 to 30.  Usual fixed pitch values are
        10 (12 cpi) and 12 (10 cpi).
 .BP    N/A
 .LQ    N/A
 .PS    ON selects proportional spacing.  Spacing tables are set up for
        a DIABLO BOLD PS wheel, #303029-01.
 .UL    Continuous underlining does not suppress microjustification
        for DWP230; does suppress it for DWP520.

TEXAS INSTRUMENTS 855 AND 865 ----- Driver: TI855

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         6    6    6 (0-8)     compressed
        10   10   10 (9-11)    elite
        12   12   12 (12-17)   pica
        14   14   -            expanded compressed
        20   20   20 (18-22)   expanded elite
        24   24   24 (23-30)   expanded pica

TOSHIBA P351, P351C, P341, P321 ----- Driver: P351

 ^PY    Selects italics
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON       Font Name
        ---  ---  ------       ---------
         7   -    -            compressed
        -    10    9 (0-9)     elite
        12   12   11 (10-14)   pica
        14   -    -            expanded compressed
        -    20   18 (15-19)   expanded elite
        24   24   22 (20-30)   expanded pica

TOSHIBA P1340 ----- Driver: P1340

 ^PY    No effect
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  Font Name
        ---  ---  ---------
        10   10   elite
        12   12   pica
        14   -    expanded compressed
        20   -    expanded elite
        24   24   expanded pica

TOSHIBA P1351 ----- Driver: P1351

 ^PY    N/A
 ^PT/V  Prints full-size characters with roll
        .LQ  .LQ
 .CW    OFF   ON  .PS ON      Font Name
        ---  ---  ------      ---------
         7   -    -           compressed
        -    10    9 (0-9)    elite
        12   12   11 (10-14)  pica
        14   -    -           expanded compressed
        -    20   18 (15-19)  expanded elite
        24   24   22 (20-30)  expanded pica

ZENITH Z-125AA ----- Driver: Z125

 ^PY    N/A
 ^PT/V  No incremental vertical positioning

 .CW    .CW  Font name
        ---  ---------
         7   16.7 cpi
         9   13.3 cpi
        10   12   cpi
        12   10   cpi
        14    8.3 cpi
        18    6.7 cpi
        20    6   cpi
        24    5   cpi

 .LH    Full lines only
 .UJ    N/A
 .PS    N/A
 .LQ    N/A
