


    This directory contains the source files of  MONGX32E MONITOR for 
    nsv-gx32-edb BOARD.
    
    FILE LIST:
    ----------
	* mongxcore.s - Main assembly source of the monitor.
	
	* def.s       - Global definitions of the monitor.
	
	* pwron.s     - Assembly source for the power-on diagnostic.
	
	* burst.c     - C source for memory test of the burst attributes.
	
	* packet.h    - Definitions of packet structure for IP, UDP and ARP
	                protocols.
			
	* header.h    - Definition for the ethernet driver.
	
	* ether.c     - C source driver of the 3COM ethernet card.
	
	* udp.c       - C source UDP protocol handler.
	
	* eserv.c     - C source to service IP, ARP and ICMP packets.
	
	* helper.s    - Assembly source for misc functions.
	
	* monio.s     - Assembly source for serial communication for debugging
	                the ethernet driver.
	
	* linkfile.rom - Monitor address map
	
	* linkfile.ram - Monitor address map for debugging the monitor.
	
	* makefile.cross - Used to compile the monitor on non native UNIX 
	                   machines.
	
	* makefile.nat   - Used to compile the monitor on native UNIX machines.
	
	* makefile.vms   - Used to compile the monitor on VMS machines with the
	                   MMS utility.
			   
	* date.c         - Time stamp of the monitor creation time.
	
	* README         - This file.
	
	
    To compile the monitor:
	
	ON UNIX:  make -f [makefile.cross | makefile.nat]
	
	ON VMS:   MMS /DES=makefile.vms
	
    The output of this is file mongx32e.hex in the INTEL HEX format
    to be burned on eprom.
    To burn this file refer to your eprom programmer manual.


