###############################################################################
#                                Info                                         #
###############################################################################

Name: 001.IMD
Aufschrift auf Diskette: 
EPC-CP/M 3.3
9x512 RamFlo
Bootfähig: Ja - Output:
CP/M V3.0 Loader
Copyright (C) 1982, Digital Research

 BNKBIOS3 SPR  F600  0600
 BNKBIOS3 SPR  A600  1A00
 RESBDOS3 SPR  F000  0600
 BNKBDOS3 SPR  7800  2E00
 
 60K TPA


SYSTEM 8013 CP/M Plus
Datentechnik oettle + reichler

??.??.??   ??:??:??   Ram: 00128k  RamDsk: 00000k

Info: HD Floppy LW mit Jumper auf 300rpm gesetzt

###############################################################################
#                           Imagedisk 1.18                                    #
###############################################################################

Settings:
Cylinders      : 80
Sides          : Two
Double-step    : Off
R/W    gap     : Calculated
Format gap     : Calculated
Format fill    : E5
Full analysis  : Yes
Interleave     : As read
Retries        : 5
Keep bad sector: Yes

   0/0: 250k DD - 9 sectors of 512 bytes - G1:24 G2:64
   0/1: 250k DD - 9 sectors of 512 bytes - G1:24 G2:64
      : Single Step

1440 Sectors (242 Compressed)

###############################################################################
#                                CP/M 3                                       #
###############################################################################

stat b: dsk:

    B: Drive Characteristics
 5616: 128 Byte Record Capacity
  702: Kilobyte Drive  Capacity
  128: 32  Byte Directory Entries
  128: Checked  Directory Entries
  128: Records/ Extent
   16: Records/ Block
   36: Sectors/ Track
    4: Reserved Tracks

A>dir b:

B: READ     ME1 : AUTODPB1 REL : AUTODSK1 REL : BIOSKRNL ASM : AUTODPB1 ASM 
B: BIOSKRN1 REL : BOOT     ASM : BNKBIOS  SUB : BNKBIOS3 SPR : BOOT1    REL 
B: BDOS3    SPR : BNKBDOS3 SPR : CALLVERS ASM : CHARIO   ASM : COPYSYS  ASM 
B: XREF     COM : CPM3     LIB : CPM3C    SYS : CPMLDR   REL : CPM3E    SYS 
B: CHARIO1  REL : COPYSYSN COM : CCP      COM : DATE     COM : DEVICE   COM 
B: DIR      COM : DIRLBL   RSX : DUMP     ASM : DUMP     COM : ED       COM 
B: ECHOVERS ASM : ERASE    COM : FD1797SD ASM : FM       COM : FORMATN  COM 
B: GENCOM   COM : GENCPM   COM : GET      COM : GENCPMC  DAT : GENCPME  DAT 
B: HELP     COM : HEXCOM   COM : HIST     UTL : HELP     HLP : INITDIR  COM 
B: LIB      COM : LINK     COM : LDRBIOS1 REL : LDRDPB1  REL : LDRDPB1  ASM 
B: LDRBIOS1 SUB : MAC      COM : MODEBAUD LIB : MOVE     ASM : PATCH    COM 
B: PIP      COM : PUT      COM : PORTS2   LIB : PORTS1   LIB : RANDOM   ASM 
B: RAMDISK1 REL : RENAME   COM : RESBDOS3 SPR : RGBTERM1 REL : RMAC     COM 
B: SHOW     COM : SAVE     COM : SCB      ASM : SET      COM : SETDEF   COM 
B: SID      COM : SUBMIT   COM : SCB      REL : TIME1    REL : TRACE    UTL 
B: TVI950   ASM : TYPE     COM : TVI950   REL : USRROUT  ASM : USRDEF1  ASM 
B: USRROUT  REL : USRDEF1  REL : XFERN    COM : Z80      LIB 
A>

###############################################################################
#                                LINUX                                        #
###############################################################################

cpmtools diskdefs:

diskdef o+r6
  seclen 512
  tracks 80
  sectrk 9
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 4
  os 2.2
end


Output linux disk-analyze:

T0.0-79.1: IBM-MFM DD (9 512-byte sectors, 4608 bytes)
T80.0-83.1: Unformatted

cpmls -f o+r6 -l -F 001.img

Directory For Drive A:  User  0

    Name     Bytes   Recs   Attributes   Prot      Update          Create
------------ ------ ------ ------------ ------ --------------  --------------

AUTODPB1 ASM    16k    126              None   
AUTODPB1 REL     2k      6              None   
AUTODSK1 REL     4k     19              None   
BDOS3    SPR    10k     77              None   
BIOSKRN1 REL     2k     11              None   
BIOSKRNL ASM    16k    125              None   
BNKBDOS3 SPR    14k    106              None   
BNKBIOS  SUB     2k      1              None   
BNKBIOS3 SPR     8k     62              None   
BOOT     ASM     4k     24              None   
BOOT1    REL     2k      8              None   
CALLVERS ASM     2k      5              None   
CCP      COM     4k     25              None   
CHARIO   ASM     6k     36              None   
CHARIO1  REL     2k     12              None   
COPYSYS  ASM    16k    117              None   
COPYSYSN COM     2k     16              None   
CPM3     LIB     4k     32              None   
CPM3C    SYS    22k    170              None   
CPM3E    SYS    22k    170              None   
CPMLDR   REL     4k     23              None   
DATE     COM     4k     23              None   
DEVICE   COM     8k     58              None   
DIR      COM    16k    114              None   
DIRLBL   RSX     2k     12              None   
DUMP     ASM     4k     32              None   
DUMP     COM     2k      8              None   
ECHOVERS ASM     2k      7              None   
ED       COM    24k    184              None   
ERASE    COM     4k     29              None   
FD1797SD ASM    12k     81              None   
FM       COM    20k    153              None   
FORMATN  COM     4k     27              None   
GENCOM   COM    16k    116              None   
GENCPM   COM    22k    168              None   
GENCPMC  DAT     4k     19              None   
GENCPME  DAT     4k     19              None   
GET      COM     8k     51              None   
HELP     COM     8k     56              None   
HELP     HLP    66k    515              None   
HEXCOM   COM     2k      9              None   
HIST     UTL     2k     10              None   
INITDIR  COM    32k    250              None   
LDRBIOS1 REL     2k     16              None   
LDRBIOS1 SUB     2k      1              None   
LDRDPB1  ASM    12k     83              None   
LDRDPB1  REL     2k      6              None   
LIB      COM     8k     56              None   
LINK     COM    16k    123              None   
MAC      COM    12k     92              None   
MODEBAUD LIB     2k      8              None   
MOVE     ASM     2k      6              None   
PATCH    COM     4k     19              None   
PIP      COM    10k     68              None   
PORTS1   LIB     4k     19              None   
PORTS2   LIB     2k     13              None   
PUT      COM     8k     55              None   
RAMDISK1 REL     2k      4              None   
RANDOM   ASM    12k     86              None   
READ     ME1    28k    214              None   
RENAME   COM     4k     23              None   
RESBDOS3 SPR     2k     16              None   
RGBTERM1 REL     4k     17              None   
RMAC     COM    14k    106              None   
SAVE     COM     2k     14              None   
SCB      ASM     4k     19              None   
SCB      REL     2k      3              None   
SET      COM    12k     81              None   
SETDEF   COM     4k     32              None   
SHOW     COM    10k     66              None   
SID      COM     8k     62              None   
SUBMIT   COM     6k     42              None   
TIME1    REL     2k      4              None   
TRACE    UTL     2k     10              None   
TVI950   ASM     4k     31              None   
TVI950   REL     2k      2              None   
TYPE     COM     4k     24              None   
USRDEF1  ASM    16k    127              None   
USRDEF1  REL     2k      6              None   
USRROUT  ASM     6k     36              None   
USRROUT  REL     2k      6              None   
XFERN    COM     2k     11              None   
XREF     COM    16k    121              None   
Z80      LIB     6k     47              None   

Total Bytes     =    611k  Total Records =    4887  Files Found =   84
Total 1k Blocks =    338   Used/Max Dir Entries For Drive A:   95/ 128
